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The FMUSER FUQ-4419R (V2) is a high-density DVB-T modulator converting IP inputs to RF outputs. It processes signals via modulation with inputs including max 1024 IP streams through 4 GE/SFP ports and 6 ASI inputs. Controlled through web-based management for seamless operation. Ideal for next-generation DTV broadcasting systems and cable headends. 
Key feature
[bookmark: OLE_LINK1]Supports high-capacity input with up to 1024 IP streams via 4 GE/SFP ports and 6 ASI inputs.  
Delivers flexible modulation for 8 or 16 DVB-T carriers compliant with ETSI EN300 744.  
Enables advanced processing including PID remapping, PCR adjustment, and PSI/SI editing.  
Features web-based management for easy configuration and monitoring.
Inner Principle Chart
For 8 carriers out:
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For 16 carriers out:
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Carrier Setting Illustration:
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Specifications
	Input
	Input
	8 DVB-T carriers: Max 512 IP input through Date1-Date4 100/1000M Ethernet Port (or SFP interface optional). Each Data port can input max 512 IP.
16 DVB-T carriers: Max 1024 IP input through Date1-Date4 100/1000M Ethernet Port (or SFP interface optional). Each Data port can input max 1024 IP.

	
	
	6 ASI input, BNC interface

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	
	Transmission Rate
	Max 840Mbps for each input channel

	Mux
	Input Channel
	512(or 1024)

	
	Output Channel
	8 (or 16)

	
	Max PIDs
	256 per channel

	
	Functions
	PID remapping(auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Modulation
Parameters
	Channel
	8(or 16)

	
	Modulation Standard
	ETSI EN300 744

	
	Constellation
	QPSK/16QAM/64QAM

	
	Bandwidth
	6/7/8 MHz

	
	Trans mode
	2K/4K/8K

	
	FEC
	1/2,2/3,3/4,5/6,7/8

	RF Output
	Interface
	F typed output port for8(or 16) non-adjacent carriers

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20~+10dbm(for all carriers), 0.5db stepping

	
	MER
	≥ 40dB

	
	ACL
	-55 dBc

	TS output
	8 (or 16) IP output over UDP/RTP/RTSP, unicast/multicast, Data1 100/1000M Ethernet Ports

	
	2 ASI output, one as mirror

	System
	Web-based Network management

	General
	Demission
	420mm×440mm×44.5mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC100V±10%, 50/60Hz or AC 220V±10%,50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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