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The FMUSER FUQ-4443 (V2) is an IP QAM modulator with inputs via 4 GE/SFP ports for up to 1024 IP streams and 6 ASI inputs. It processes signals by modulating them into 16 or 32 non-adjacent DVB-C carriers. Featuring web-based network management, this device is ideal for cost-effective DTV broadcasting systems. 
Key feature
Enables web-based network management for remote monitoring and control.
Principle Chart
For 16 carriers out:
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For 32 carriers out:
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Carrier Setting Illustration:
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Specifications
	Input
	Input
	16/32 DVB-C carriers: Max 1024 IP input through Date1-Date4 100/1000M Ethernet Port (or SFP interface optional). Each Data port can input max 1024 IP.

	
	
	6 ASI input, BNC interface

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	
	Transmission Rate
	Max 840Mbps for each GE input

	Mux
	Input Channel
	1024

	
	Output Channel
	16/32

	
	Max PIDs
	256 per channel

	
	Functions
	PID remapping(auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Scrambling
Parameters
	Max simulscrypt CA
	6

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
Parameters
	DVB-C Modulator Section
	J.83A
	Constellation : 16/32/64/128/256QAM

	
	
	
	Bandwidth :8M

	
	
	J.83B
	Constellation : 64QAM/ 256QAM

	
	
	
	[bookmark: OLE_LINK5]Bandwidth :6M

	
	QAM Channel
	16/32 non-adjacent carrier

	
	Modulation Standard
	EN300 429/ITU-T J.83A/B(DVB-C)

	
	Symbol Rate
	5.0~7.0Msps, 1ksps stepping

	
	Constellation
	16, 32, 64 , 128, 256QAM

	
	FEC
	RS (204, 188)

	RF Output
	Interface
	1 F typed output port for 16/32 carriers, 75Ω

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20dBm~+10dBm(87~117dbµV), 0.1dB stepping

	
	MER
	≥ 40dB

	TS output
	16/32 IP output over UDP/RTP/RTSP, unicast/multicast, Data1 100/1000M Ethernet Ports

	
	2 ASI output, one as mirror

	System
	Network management software (NMS) supporting

	General
	Demission
	420mm×440mm×44.5mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz or AC 220V±10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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