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The FUQ-4454B-C is a 1RU 4-in-1 mux-scrambling encoder modulator with 4× CVBS/YPbPr/S-Video inputs, 1-2× DVB-C tuners, and 2× IP interfaces. It performs MPEG-2 encoding, ETSI-compliant scrambling, and 16-256QAM modulation in a single pass. The unit features 30–999 MHz RF output with web/USB management and complies with DVB-C (EN300 429) and ITU-T J.83A/B/C. Ideal for CATV digital migration and IPTV edge QAM deployments.
Key feature
Modular upgradability: Features pluggable modules and dual web/USB control for future-proof operation.
 
Specifications
 
	Input
	1 or 2 DVB-C Tuner input for remux; 2 IP input for re-mux

	
	4 CVBS/YPbPr/S-Video Input for encoding

	Tuner Input
	DVB-C
	Standard
	J.83A(DVB-C), J.83B, J.83C

	
	
	Input Frequency
	30MHz-1000Mhz

	
	
	Constellation
	16/32/64/128/256 QAM

	Encoding
	Video
	Format
	MPEG-2 MP@ML (4:2:0)

	
	
	Interface
	S-Video/YPbPr/CVBS*4

	
	
	Bitrate
	1-19.5Mbps

	
	
	Resolution
	720*480_60i, 720*576_50i

	
	
	Rate mode
	VBR/CBR

	
	
	Chroma
	4:2:0

	
	
	Aspect
	16:9,4:3, 1:1, 2.21:1

	
	Audio
	Format
	MPEG1 Layer II, AC3

	
	
	Sampling
	48KHz

	
	
	Bitrate
	64kbps,96kbps,128kbps,192kbps,256kbps,320kbps

	Multiplexing
	Maximum PID Remapping
	128per input channel

	
	Function
	PID remapping (automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/SI table automatically

	Scrambling
	Maximum simulcrypt CA
	4

	
	Standard
	ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	QAM Channel
	4

	
	Standard
	EN300 429/ITU-T J.83A/B/C

	
	MER
	≥40db

	
	RF frequency
	30~999MHz, 1KHz step

	
	RF output level
	-20~0dbm(87~107 dbµV),0.1db step

	
	Symbol Rate
	5.0Msps~9.0Msps, 1ksps stepping

	
	Constellation
	16/32/64/128/256QAM

	
	 
	J.83A
	J.83B
	J.83C

	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM
	64/256 QAM

	
	Bandwidth
	8M
	6M
	6M

	System
	Local interface
	LCD + control buttons

	
	Remote management
	Web NMS

	
	Stream Out
	4*MPTS IP over UDP out (RJ45, 1000M, Unicast/Multicast)

	
	Language
	English

	
	Software Upgrading
	Web and USB port

	General
	Dimension
(W*D*H)
	482mm×300mm×44.5mm

	
	Weight
	3.7kg

	
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power
	AC 100V±1050/60Hz;
AC 220V±10%, 50/60HZ

	
	Consumption
	25W


 
Working Principle
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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