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The FUQ-4455B IP QAM Modulator integrates multiplexing, scrambling, and modulation, processing 192 IP inputs via 4×FE and 1×GE ports to output 4 DVB-C RF carriers. It handles SPTS/MPTS streams using UDP/RTP, with PID remapping and PSI/SI editing for compliance. Features web-based control and USB upgrades in a compact chassis. Ideal for IPTV systems and cable TV headends, enabling flexible integration.
Key Features
Handles High-Capacity IP Inputs: Supports 192 SPTS/MPTS streams via UDP/RTP with 4×FE and 1×GE ports.FMUSER FUQ-4455B IP QAM Modulator 192 IP Inputs UDP-RTP DVB-C EN300-429 ITU-T J.83 A-B-C PID Remapping PCR Adjusting IPTV Cable TV HeadendSupports Precision Signal Control: Enables PID remapping, PCR adjusting, and PSI/SI editing for DVB-C standards.FMUSER FUQ-4455B IP QAM Modulator 192 IP Inputs UDP-RTP DVB-C EN300-429 ITU-T J.83 A-B-C PID Remapping PCR Adjusting IPTV Cable TV HeadendGenerates Multi-Standard RF Output: Delivers 4 adjacent QAM carriers (30MHz–1000MHz) meeting EN 300 429/ITU-T J.83 A/B/C.FMUSER FUQ-4455B IP QAM Modulator 192 IP Inputs UDP-RTP DVB-C EN300-429 ITU-T J.83 A-B-C PID Remapping PCR Adjusting IPTV Cable TV HeadendFeatures Unified Management: Includes web-based control, USB upgrades, and IPTV Sync/NTP synchronization.   
Working Principle
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Specifications
 
	Input
	128 IP (SPTS/MPTS) input over UDP/RTP, 4*100M Ethernet port, and
64 IP (SPTS/MPTS) input over UDP/RTP, 1*100/1000M Ethernet ports

	Multiplexing
	Maximum PID Remapping
	748 per input channel

	
	Function
	PID remapping (automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/SI table automatically

	Scrambling
	Maximum simulcrypt CA
	4

	
	Standard
	ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	QAM Channel
	1 F typed output port for 4 carriers, 75Ω

	
	Standard
	EN300 429/ITU-T J.83A/B/C

	
	MER
	≥40db

	
	RF Frequency
	30~1000 MHz, 1kHz stepping

	
	RF Output level
	-10dBm~+0dBm, 0.1dB stepping

	
	FEC
	RS (204, 188)

	
	Symbol Rate
	5.0Msps~9.0Msps, 1ksps stepping

	
	 
	J.83A
	J.83B
	J.83C

	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM
	64/256 QAM

	
	Bandwidth
	8M
	6M
	6M

	Stream Out
	4 IP (SPTS/MPTS) output over UDP, 1*1000M Ethernet port (IPTV Port)

	System
	Web-based Network management

	
	Chinese and English Language

	
	Web and USB software upgrade

	General
	Dimension
	430mm×180mm×44mm (W*L*H)

	
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power
	AC 100V±1050/60Hz; AC 220V±10%, 50/60HZ


 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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