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The FMUSER FUQ-4475 modulator converts IP signals to RF outputs, supporting up to 512 IP inputs via 6 GE ports and 64 QAM carriers through dual RF interfaces. It processes streams with multiplexing, scrambling, and modulation to DVB-C standards. Featuring web-based management, this device is ideal for broadcast headends and cable television distribution systems. 
Key feature
       Enables web-based control for network configuration. 
Inner Principle Chart
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Carrier Setting Illustration
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Specifications
	Input
	Input
	Max 512 IP inputs from 6*100/1000M Ethernet Port   (4*RJ45, 2*SFP)

	
	Transport Protocol
	TS over UDP/RTP, unicast and multicast, IGMP V2/V3

	
	Transmission Rate
	Max 840Mbps for each GE input

	Mux
	Input Channel
	512

	
	Output Channel
	64

	
	Max PIDs
	256 per channel

	
	Functions
	PID remapping(auto/manually optional)

	
	
	PCR accurate adjusting

	
	
	PSI/SI table automatically generating

	Scrambling
Parameters
	Max simulscrypt CA
	6

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
Parameters
	Modulation Standard
	  EN300 429/ITU-T J.83A/B/C

	
	Constellation
	J.83A
	Constellation :16/32/64/128/256QAM

	
	
	
	Bandwidth :8M

	
	
	J.83B/C
	Constellation :64/256QAM

	
	
	
	Bandwidth :6M

	
	QAM Channel
	64 non-adjacent carriers
384Mbps bandwidth for each RF interface

	
	Symbol Rate
	5.0~7.0Msps, 1ksps stepping
5057Ksps (J.83B, 64QAM) ; 5361Ksps (J.83B, 256QAM)

	
	Constellation
	16, 32, 64 , 128, 256QAM

	
	FEC
	RS (204, 188)

	RF Output
	Interface
	2 F type output ports for 64 carriers, 75Ω

	
	RF Range
	50~960MHz, 1kHz stepping

	
	Output Level
	-20dBm~+10dBm(87~117dbµV), 0.1dB stepping

	
	MER
	≥ 40dB

	TS output
	64 IP output over UDP/RTP/RTSP, unicast/multicast, 4*100/1000M Ethernet Ports (each port for 16 IP outputs)

	System
	Web-based Network management

	General
	Demission
	420mm×440mm×44.5mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC 100V±10%, 50/60Hz or AC 220V±10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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