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The FMUSER FUQ-4515 is a two-way DVB-S2 satellite modem for efficient IP data transmission over satellite. It modulates and demodulates IP signals using TCP acceleration to optimize performance. Featuring web-based NMS with LCD and keyboard support, it simplifies management. Ideal for satellite networks in broadcast, enterprise, and remote data services. 
Key feature
Supports DVB-S2 and legacy DVB-S standards for efficient satellite communication.
Embedded TCP acceleration optimizes high-speed links and heavy traffic.
High throughput up to 100 Mbps for upstream and downstream operations.
Web-based NMS operation with LCD and keyboard support for easy management. 
Principle Chart
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Specifications
 
	Input/Output
	IP input/output over IPv4 (TCP/UDP/ICMP…) protocol
1 tuner in and 1 RF out

	Tuner Section
	DVB-S2
	Input Frequency
	950-2150MHz

	
	
	Symbol rate
	QPSK 1~45Mbauds;
8PSK 2~30Mbauds

	
	
	Code rate
	1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	Constellation
	QPSK, 8PSK

	RF output
	RF Range
	950 ~ 2150 MHz, 10KHz step

	
	Output Level Attenuation
	0 dBm~-31.5 dBm, 0.5dB Step

	
	MER
	≥40dB

	
	Connector
	N type, impedance 50Ω

	 
 
 
 
 
Modulation
 
	Standard
	DVB-S2

	
	Outer coding
	BCH Coding

	
	Inner coding
	LDPC Coding

	
	Constellation
	QPSK,8PSK,16APSK,32APSK

	
	FEC/ Convolution Rate
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	Roll-off Factor
	0.2, 0.25, 0.35

	
	Symbol Rate
	0.05~40Msps (32APSK);
0.05~45Msps (QPSK/8PSK/16APSK)

	System
	LCD/keyboard operating, web-based NMS manage

	
	Language: English/Chinese

	
	Ethernet software & hardware upgrade

	Miscellaneous
	Dimension
	482mm×328mm×44mm (W× L× H)

	
	Temperature
	0~45℃ (work),  -20~80℃（Storage）

	
	Power
	AC 100V-220V±10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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