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The FMUSER FUQ-4618Px is a 1U modular IP Gateway converting IP streams to DVB-ASI via 3 hot-swappable cards. Each card processes 512 SPTS/MPTS streams through UDP/RTP with CA filtering and PCR correction. Features dual Gigabit Ethernet ports (1 input + 1 output) and web-based PSI/SI editing. Ideal for broadcast headends, CATV systems, and IP contribution networks requiring high-density conversion.
 
Key feature
Low 20W power consumption with 0-45°C operating temperature range 
Specifications
	Input
	512 SPTS or MPTS IP input over UDP, RTP, Unicast and Multicast (per card)

	Output
	512 SPTS IP output UDP, RTP, Unicast and Multicast (per card)

	Multiplexing
	Support CA PID filtering, PID re-mapping

	
	Support accurate PCR adjusting

	
	Support PSI/SI rebuilding and editing

	General
	Dimension(WxLxH)
	482mm×410mm×44mm

	
	Weight
	3.6kg

	
	Temperature
	0~45℃(working )，-20~80℃(storage)

	
	Power supply
	100~240VAC，50/60Hz

	
	consumption
	20W


 
Working Principle (per daughter card)
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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