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The FUQ-4618Ry is a 12-channel IP-to-ASI gateway converting UDP/IP streams to DVB-ASI via dual Gigabit Ethernet inputs (RJ45/SFP). It processes MPTS/SPTS with PCR timing restoration and jitter correction for stable TS streams. The 1U rack-mount unit supports local LCD control and SNMP monitoring. Ideal for broadcast headends requiring high-density IP migration and cable TV systems upgrading legacy ASI infrastructure. 
Key feature
Offers local LCD/keypad control and SNMP remote monitoring
Specifications
	Interface
	Input
	12 IP (MPTS/SPTS)over UDP, unicast and multicast, two 1000M input interfaces, RJ45/SFP

	
	Output
	12 ASI output, and each channel output with two BNC interfaces

	Transmitting protocol
	Input
	TS over UDP

	
	Output
	DVB-ASI

	Bit-rate
	Max of each channel is 108Mbps, Max total bit-rate is 840Mbps

	Miscellaneous
	Dimension
(W×L×H)
	482mm×410mm×44mm

	
	Weight
	4kg

	
	Temperature
	0~45℃(operation)，-20~80℃(storage)

	
	Power
	100~240VAC，50/60Hz

	
	Consumption
	22W


 
Principle chart
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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