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FUQ-4618SY 12-Channel IP to ASI Gateway with Dual Gigabit Inputs/DVB-ASI Outputs for Broadcast Transmission [image: 3EEECN_20180827064931]
Product overview
The FUQ-4618SY converts UDP/IP streams to DVB-ASI signals via 12 output channels, each with dual BNC interfaces. It processes MPTS/SPTS inputs through dual Gigabit Ethernet ports (RJ45/SFP), ensuring 840Mbps throughput with PCR restoration. This 1U rack-mount device supports SNMP/LCD control for broadcast centers and IPTV headends requiring stable TS stream conversion.
Key feature
Remote management via SNMP or local LCD controlSpecifications
	Interface
	Input
	12 IP (MPTS/SPTS)over UDP, unicast and multicast, two 1000M input interfaces, RJ45/SFP

	
	Output
	12 ASI output, and each channel output with two BNC interfaces

	Transmitting protocol
	Input
	TS over UDP

	
	Output
	DVB-ASI

	Bit-rate
	Max of each channel is 108Mbps, Max total bit-rate is 840Mbps

	Miscellaneous
	Dimension
(W×L×H)
	482mm×410mm×44mm

	
	Weight
	4kg

	
	Temperature
	0~45℃(operation)，-20~80℃(storage)

	
	Power
	100~240VAC，50/60Hz

	
	Consumption
	22W
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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