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Product overview
The FMUSER FUQ-4619A/FUQ-4619B IPTV Gateway Server integrates an IP Gateway and IPTV server for protocol conversion and streaming media distribution. It handles inputs such as SRT, HTTP, UDP, RTP, RTSP, and HLS, converting to outputs including SRT, HTTP, UDP, HLS, and RTMP. Managed via web-based NMS through the DATA port, it suits small CATV headend systems and hotel TV applications for efficient media delivery. 
Key feature
Integrated Design: Combines IP Gateway and IPTV server in one unit for streamlined operation.  
Protocol Conversion: Converts inputs like SRT, HTTP, UDP, RTP, RTSP, and HLS to outputs such as SRT, HTTP, UDP, HLS, and RTMP.  
IPTV Functionality: Supports live channels, VOD, hotel services, and customizable interfaces via FMUSER IPTV APK.  
Web Management: Controlled through web-based NMS for easy configuration and monitoring. 
IP Protocol Conversion
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General Principle Chart
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Specifications
	 IP Input
	DATA CH 1-7 (1000M) ports: IP input over SRT, HTTP, UDP (SPTS), RTP (SPTS), RTSP (over UDP, payload: mpeg TS) and HLS

	
	TS files uploading through Web management

	IP output
	First Data port (1000M): IP out over SRT, HTTP (Unicast), UDP (SPTS, Multicast) HLS and RTMP (Program source should be H.264 and AAC encoding)

	
	DATA CH 1-7 (1000M) ports: IP out over HTTP/HLS/RTMP (Unicast)
SFP+ output 10000M (for FU-4619S-I and FU-4619I)

	System
	Channel switching time with FMUSER’ STB: HTTP (1-3s), HLS (0.4-0.7s)

	
	Play programs with APK downloaded android STB and TV

	
	About 80 HD/SD programs (Bitrate at 2Mbps) when HTTP/RTP/RTSP/HLS is converted into UDP (Multicast), the actual application shall prevail, and suggest maximum 80% CPU utilization

	
	IPTV system function
	support Live channel, VOD, Hotel introduction, Dining, Hotel service, APPS, scenery introduction and so on (Please install FMUSER IPTV APK)

	
	IPTV system main interface
	support adding scrolling caption, welcome words, pictures, advertisement, video, music (Please install FMUSER IPTV APK)

	
	web-based NMS management thru DATA port

	General
	Demission
	482.6mm×328mm×88mm (WxLxH)

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power Supply
	AC100V±10%, 50/60Hz or AC 220V±10%, 50/60Hz


 
Test data for reference:
	[bookmark: OLE_LINK30]Protocol Conversion
	Programs
	Bitrate
	Terminals
	CPU Utilization

	
	
	
	FU-4619S-M
	FU-4619I
	

	HTTP/RTP/RTSP/HLS to UDP
	80
	2M
	---
	---
	55%

	HTTP to HTTP
	30
	2M
	300
	600
	80%

	
	50
	2M
	160
	320
	80%

	HTTP to HLS
	50
	2M
	400
	800
	46%

	UDP to HLS
	50
	2M
	400
	800
	50%

	
	80
	2M
	300
	600
	72%

	UDP to HTTP
	50
	2M
	240
	480
	50%

	UDP to SRT
	50
	2M
	---
	---
	50%

	UDP to SRT
	50
	2M
	---
	---
	75%


 
Order Guide:
	Model No.
	Feature
	SFP+
	Memory
	CPU
	Solid-State Disk (SSD)
	Mechanical Hard Disk

	FU-4619F-M
	Gateway+IPTV server
	/
	8G
	i5/i7 (3rd Generation)
	120G/240G random
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	FU-4619S-M
	Gateway+IPTV server
	/
	8G
	i5/i7 (3rd Generation)
	120G/240G random
	4T

	FU-4619S-I
	Gateway+IPTV server
	1
	8G
	i3 (6th Generation)
	[bookmark: OLE_LINK1]120G/240G random
	/

	FU-4619I
	Gateway+IPTV server
	1
	16G
	i7 (6th Generation)
	120G/240G random
	4T


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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