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The FMUSER FUQ-4619C V2 is a tuner to IP gateway with 16 tuner inputs and 2 ASI inputs for IP MPTS output. It multiplexes signals and applies BISS descrambling with PSI/SI management. Controlled via web interface, it suits digital TV head-end systems for broadcasting.   
Key feature
Supports up to 16 tuner inputs with DVB-S/S2/S2X standards and 2 ASI inputs.  
Features embedded BISS descrambling with bit rate up to 80Mbps per channel.  
Provides 4 IP outputs over UDP/RTP/RTSP and 2 GE mirrored outputs.  
Enables PID filtering, re-mapping, and PSI/SI editing.  
Working Principle
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Specifications
 
	Input
	16 tuners input, (DVB-C, DVB-T/(T), ISDBT, S/S2/S2X, ATSC optional), F type
2 ASI input, BNC interface

	Tuner Section
	 
	DVB-C
	Input Frequency
	30 ~1000 MHz

	
	
	
	Standard
	J.83A(DVB-C), J.83B, J.83C

	
	
	
	Constellation
	16/32/64/128/256 QAM

	
	 
	DVB-T/(T)
	Input Frequency
	30 ~1000 MHz

	
	
	
	Bandwidth
	6/7/8 M

	
	Version 1
	DVB-S
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	1~45 Msps

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	
	Signal Strength
	- 65~ -25dBm

	
	
	
	Max input bitrate
	≤120 Mbps

	
	
	DVB-S2
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	1~45 Msps

	
	
	
	FEC
	1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK

	
	
	
	Max input bitrate
	≤120 Mbps

	
	Version 2
(New)
	DVB-S
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	0.5~45Msps

	
	
	
	Signal Strength
	- 65- -25dBm

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	
	Max input bitrate
	≤120 Mbps

	
	
	DVB-S2
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~40Msps;

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                           
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10                                            
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                          
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤120 Mbps

	
	
	DVB-S2X
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK/32APSK: 0.5~40Msps

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤120 Mbps

	
	 
	ISDB-T
	Input Frequency
	30~1000MHz

	
	 
	ATSC
	Input Frequency
	50 MHz~960MHz

	
	
	
	Bandwidth
	6M

	
	
	
	Constellation
	8VSB

	Re-multiplex
	PID re-mapping

	
	PCR accurate adjusting

	
	Automatic generating PSI/SI table

	PID
	Output range
	0x0000—0x1FFF

	
	PID transparent
	Any PID transparent and mapping achievable

	
	Amount of output PID per input
	128

	BISS descrambling
	Mode 1, Mode E (Up to 850Mbps) (descramble individual program)

	Output
	4 IP (MPTS) output over UDP and RTP/RTSP protocol through GE1 and GE2 port, Unicast and Multicast

	System
	Remote management
	Web-server Management

	
	Language
	English

	
	Upgrade
	USB, web management

	Miscellaneous
	Dimension
	482mm×410mm×44mm   (W×L×H)

	
	Approx weight 
	3.5kg

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements 
	100~240VAC, 50/60Hz

	
	Power consumption 
	20W


 
 
 
Tuner Input Options:
 
	· 8 DVB-C Tuners + 8 ATSC Tuners

	· 8 DVB-S2/S2X Tuners + 8 DVB-(T) Tuners

	· 8 DVB- S2/S2X Tuners + 8 ISDB-T Tuners

	· 16 DVB-S/S2/S2X/DVB-C/(T) /ISDB-T/ATSC Tuners


 
 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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