[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[bookmark: _GoBack]FUQ-4619C Tuner to IP Gateway 24 Tuners 2 ASI 1 USB Inputs DVB-S-S2-S2X DVB-C-T-T2 ISDB-T 1024 SPTS 27 MPTS IP Streaming BISS Descrambling Web GUI Broadcast Headend [image: 3EEECN_20240131172127]Product overview
The FUQ-4619C Tuner to IP Gateway converts signals from 24 FTA tuners, 2 DVB-ASI inputs, and 1 USB input into IP outputs. It processes signals with switchable MPTS (bypass) or SPTS modes and embedded BISS descrambling. Managed via Web GUI, it delivers up to 1024 SPTS streams over UDP/RTP/RTSP. This 1RU device is ideal for broadcast headends and IPTV distribution requiring flexible signal conversion. 
Key feature
Supports 24 multi-standard tuners (switchable DVB-S/S2/S2X, DVB-C/T/T2, ISDB-T) plus 2 ASI inputs and 1 USB input.
Integrates BISS descrambling for Mode 1 and Mode E on tuner inputs.
Provides switchable MPTS/SPTS outputs (27 MPTS with Null PKT Filter or 1024 SPTS over dual DATA ports via UDP/RTP/RTSP).
Enables Web-based management for configuration, PID filtering, remapping, and updates.
Includes DiSEqC support for satellite signal control.
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Specifications
	Input
	24 tuners inputs +2 ASI inputs +1 USB inputs

	Satellite
	DVB-S
	Frequency In
	950~2150MHz

	
	
	Symbol rate
	0.5~45Msps

	
	
	Signal Strength
	- 65- -25dBm

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	Constellation
	QPSK

	
	
	Max input bitrate
	≤125 Mbps

	
	DVB-S2
	Frequency In
	950~2150MHz

	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~34Msps;

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	Max input bitrate
	≤125 Mbps

	
	DVB-S2X
	Frequency In
	950~2150MHz

	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~34Msps

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10, 2/3-L, 32/45, 11/15, 7/9

	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	Max input bitrate
	≤125 Mbps

	Multi-Mode Switchable Tuner Inputs
	DVB-C
	Standard
	J.83A(DVB-C), J.83B, J.83C

	
	
	Frequency In
	50~960MHz

	
	
	Constellation
	16/32/64/128/256 QAM

	
	DVB-T/T2
	Frequency In
	50~960MHz

	
	
	Bandwidth
	6/7/8 M bandwidth

	
	ISDB-T
	Frequency In
	50~960MHz

	BISS Descrambling
	Mode 1, Mode E

	Output
	1024 SPTS IP output over UDP and RTP/RTSP protocol through DATA1 and DATA2 port (IP address and port number of DATA1 and DATA2 are different) , Unicast and Multicast

	
	27 MPTS IP output (for Tuner/ASI/USB bypass) over UDP and RTP/RTSP protocol through DATA1 and DATA2 port, Unicast and Multicast

	
	2 ASI outputs(MPTS out mode only, mirror ports to output the same one TS)

	System
	Web based management

	
	Ethernet software upgrade

	Miscellaneous
	Dimension
	482mm×270mm×44mm (W×L×H)

	
	Environment
	0~45℃(work); -20~80℃（Storage）

	
	Power requirements  
	100~240VAC, 50/60Hz


 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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