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The FUQ-4619C Tuner-to-IP Gateway converts 16-24 DVB-S/S2/S2X tuner inputs, 1 ASI, and 1 USB signals into IP streams via UDP/RTP/RTSP. It processes signals with BISS descrambling, DiSEqC control, and PID filtering, delivering up to 26 MPTS or 1024 SPTS streams through dual Gigabit Ethernet ports. This 1RU rack-mountable device features web-based management, ideal for broadcast headends and IPTV multiscreen distribution. 
Key feature
Web-based configuration and Ethernet firmware upgrades for remote management 
Working Principle
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Specifications
	Input
	16 or 24 tuners input +1 ASI input +1 USB input---SPTS/MPTS output

	Satellite
	DVB-S
	Frequency In
	950~2150MHz

	
	
	Symbol rate
	0.5~45Msps

	
	
	Signal Strength
	- 65- -25dBm

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	Constellation
	QPSK

	
	
	Max input bitrate
	≤125 Mbps

	
	DVB-S2
	Frequency In
	950~2150MHz

	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~34Msps;

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	Max input bitrate
	≤125 Mbps

	
	DVB-S2X
	Frequency In
	950~2150MHz

	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~34Msps

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10, 2/3-L, 32/45, 11/15, 7/9

	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	Max input bitrate
	≤125 Mbps

	BISS Descrambling
	Mode 1, Mode E (Up to 850Mbps) (descramble individual program)

	Output
	1024 SPTS IP output over UDP and RTP/RTSP protocol through GE1 and GE2 port (IP address and port number of GE1 and GE2 are different) , Unicast and Multicast

	
	26 MPTS IP output (for Tuner/ASI/USB pass-through) over UDP and RTP/RTSP protocol through GE1 and GE2 port, Unicast and Multicast

	
	2 ASI output

	System
	Web based management

	
	Ethernet software upgrade

	Miscellaneous
	Dimension
	482mm×230mm×44mm (W×L×H)

	
	Approx weight  
	2.5 kg

	
	Environment
	0~45℃(work); -20~80℃（Storage）

	
	Power requirements  
	100~240VAC, 50/60Hz

	
	Power consumption  
	20W


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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