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The FMUSER FUQ-4619C V3 converts 24 RF tuner inputs to IP streams via UDP/RTP output. It processes DVB-T/T2/C/S/S2 signals with QPSK/QAM/COFDM modulation. This 1RU rack-mount device features web-based NMS control. Ideal for broadcasters transitioning to IP infrastructure and multi-format headend systems.It has the functions of supporting auto-generation of PSI/SI information, PID re-mapping, service filtering and PCR adjusting. In conclusion, its high integration and cost effective design make this device widely used in the CATV Broadcasting system.
 
Key feature
1RU rack-mount design with 10/100/1000Mbps Ethernet 
Inner Principle Chart
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Specifications
	Input / Output
	4 bi-direction ASI ports: max 4 ASI input/output, BNC 75Ω
3 bi-direction Data ports (RJ45): 128 IP input over UDP/RTP
4 IP (MPTS) output over UDP/RTP/RTSP
100/1000Mbps self-adaption

	
	Input Packet format: 204/188 self-adaption

	
	ASI: Max output bit-rate: 200Mbps (Each channel)

	Mux
	Max PIDs
	512 per channel

	
	Functions
	PID re-mapping

	
	
	PCR accurate adjusting

	
	
	Automatic generating PSI/SI table

	
	PID transparent
	Any PID transparent and mapping achievable

	Scrambling
Parameters
	Max simulcrypt CA
	4

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Scramble Channel
	1

	
	Connection
	Local/remote connection

	System
	Web-based management

	
	Language: English and Chinese

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×300mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz

	
	Consumption
	≤40W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.

   Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227

image2.jpeg
DEOING
DX3514 Multiplexer Scrambler





image3.jpeg
TS output #1
(ASI1&IP1

ASIIN #1
ASI1&IP1

ASI IN #2 TS output #2
ASI IN #3 ASI2 &IP 2
TS output #3

ASI IN #4 (ASI3 &IP3

) ASI3 &IP3
128 IP IN )

TS output #4

ASI4 &IP 4

ASI direction can be defined as input or output




image1.png
FMuser




