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Product overview
The FMUSER FUQ-4633 HD Encoder Modulator integrates 1 HDMI input and RF output with MPEG-4 AVC/H.264 encoding and DVB-T modulation. It processes audio/video signals by encoding and modulating them for RF transmission. This device is ideal for home entertainment, surveillance systems, and commercial applications like hotel digital signage.
 Key feature
- Supports H.264 video encoding with auto detect for MP@L 3.0/3.1/4.0.  
- Features MPEG-1 Layer 2 and MPEG-2 AAC audio encoding.  
- Provides RF output at 142.5-858 MHz with adjustable level from -14 to +6 dBm.  
- Includes 1 HDMI input for simplified source connectivity.  
- Enables system upgrades via USB port with external disk support.  
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System Connection
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Technical Specifications
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Typical Applications
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Main Technical Comparison between FU-4633 and FU-4667 (HD, DVB-T Version)
	Items
	FU-4633
	FU-4667 (HD, DVB-T )

	Interface
	HDMI
	HDMI/YPbPr/CVBS/S-Video

	Video Encoding
	H.264 MP@L 3.0/3.1/4.0
Auto detect and configure
	H.264 BP/MP/HP@L 3.0/3.1/3.2/4.0/4.1/4.2
Profile and level can be manually set

	Resolutions
	Input and output scanning format and frame rate change
	Input and output scanning format and frame rate keep the same

	Audio Encoding
	MPEGI layer 2, MPEG-2 AAC
	MPEG1 Layer II, MPEG2-AAC, MPEG4-AAC

	MER
	≥31dB
	≥42dB

	RF Frequency
	142.5~858 MHz
	30~960MHz

	Output Level
	-14~ +6dBm
	-16~ -36dBm

	USB (External USB Disk)
	System upgrade
	System upgrade, TS record and playback


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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HDMI Encoding Section

Constellation QPSK, 16QAM, 640AM

Encoding H.264 MP@L 3.0/3.1/4.0 Code rate 1/2,2/3,3/4,5/6,7/8
Interface HDOMI*L Guard Interval 1/32,1/16,1/8, 1/4
Input Output Transmission Mode: 2K, 8K
480@59.94/60i 480@30p MER 231d8
760501 s76@250 RF frequency 142.57858 MHz, 1KHz step
Video 720@50/59.94/60p 720@50/59.94/60p RF output level -14~ +6dBm, 0.1db step
Resolution
1080@501 1080@25p System
1080@59.94/60i 1080@30p RF mix in ATT 10dB
1080@59.94/60p 1080@30p Management Local LCD + control buttons
AspectRatio 169, 4:3 Language English
Bit rate 1.000~18.000 Mbps LCN Insertion yes
Encoding MPEGI layer 2 Upgrade UsB
Audio | samplerate  48KHz General
Bit rate 64, 96,128, 192, 256, 320kbps Power supply DC 12V
DVB-T Modulator Section Dimensions 153*110*50mm
Standard DVB-T COFDM Weight <1kg
Bandwidth 6M, 7M, 8M
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