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FMUSER FUQ-4633B HD Encoder Modulator HDMI Input to RF Output MPEG2 Encoding Multi-Standard DVB-C-T-ATSC-ISDB-T Modulation Web-NMS Control for TV Distribution and Surveillance
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Product overview
The FMUSER FUQ-4633D is an HD Encoder Modulator that accepts HDMI input signals and outputs RF signals. It performs MPEG2 encoding and modulation to convert audio/video signals into broadcast-ready formats. Available in compact sizes (e.g., 20314452mm or 18011039.5mm), it supports management via Web or NMS. Ideal for TV distribution in home entertainment, surveillance, and commercial applications.
Key feature
Supports MPEG2 video encoding at 1.000-20.000 Mbps and audio in MPEG1 layer 2, AAC, AC3 formats.  
Features multi-standard modulation including DVB-C, DVB-T, ATSC, ISDB-T with RF frequency 100-1000MHz and level -63 to -16dBm.  
Offers flexible management via Web or NMS, with upgrade options.  
Accepts HDMI input from sources like STBs, satellite receivers, CCTV cameras.  
Compact design with dimensions 20314452mm or 18011039.5mm for space efficiency. 
System Connection
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Technical Specifications
	HDMI Encoding Section

	Video
	Encoding
	MPEG2

	
	Interface
	HDMI*1

	
	Input
	Output

	
	480@59.94/60i
	480@30p

	
	576@50i
	576@25p

	
	720@50/59.94/60p
	720@25/30p

	
	1080@50i
	1080@25p

	
	1080@59.94/60i
	1080@30p

	
	1080@50p
	1080@25p

	
	1080@59.94/60p
	1080@30p

	
	Aspect Ratio
	16:9

	
	Bit rate
	1.000~20.000 Mbps

	Audio
	Encoding
	MPEGI layer 2, AAC, AC3

	
	Sample rate    48KHz

	
	Bit rate
	MPEGI layer 2（192kbps）

	
	
	AAC（VBR）

	
	
	AC3（128kbps）

	DVB-C Modulator Section

	Standard
	J.83A (DVB-C), J.83B

	MER
	≥35dB

	RF frequency
	100-1000MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	Symbol rate
	3.000~7.000Msps adjustable

	 
	J.83A
	J.83B

	Constellation
	16/32/64/128/ 256 QAM
	64/ 256 QAM

	Bandwidth
	8M
	6M

	DVB-T Modulator Section

	Standard
	DVB-T COFDM

	Bandwidth
	2M, 3M, 4M, 5M, 6M, 7M, 8M (Version—Ⅰ)
6M, 7M, 8M (Version—Ⅱ)

	Constellation
	QPSK, 16QAM, 64QAM

	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	Guard Interval
	1/32, 1/16, 1/8, 1/4

	Transmission Mode:
	2K, 8K

	MER
	≥35dB

	RF frequency
	100-1000MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	ISDB Modulator Section

	Standard
	ARIB STD-B31

	Constellation  
	QPSK, 16QAM, 64QAM

	Guard Interval
	1/32, 1/16, 1/8, 1/4

	Transmission Mode
	2K, 4K, 8K

	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	RF frequency
	100~1000MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	ATSC Modulator Section

	Standard
	ATSC A/53

	Constellation
	8 VSB

	RF output level
	-63~-16dBm (44~91 dBµV), 1dB step

	MER
	≥35dB

	RF frequency
	100~1000MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	System

	Management
	Web (Version—Ⅰ)
NMS (Version—Ⅱ)

	Language
	English

	Upgrade
	Web update (Version—Ⅰ)
ST Link utility (Version—Ⅱ)

	General

	Power supply
	DC 12V

	Dimensions
	203*144*52mm (Version—Ⅰ)
180*110*39.5mm (Version—Ⅱ)

	Weight
	< 1kg


 
Comparison
	Device
	CC input
	Management
	Upgrade

	FU-4633C (Version—Ⅰ)
	√
	Web
	Web

	FU-4633C (Version—Ⅱ)
	Optional
	NMS
	ST Link utility
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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