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Product overview 
 The FMUSER FUQ-4633C is an HD/SD encoder modulator that accepts HDMI and CVBS inputs and outputs ISDB-T or DVB-T RF signals. It encodes video using H.264 MPEG-4 AVC and modulates for RF transmission. With local LCD control and USB upgrade, it supports easy configuration. Ideal for home entertainment, surveillance systems, and digital signage broadcasting. 
Key feature
- Supports dual-standard modulation: ISDB-T (ARIB STD-B31) and DVB-T (COFDM) with 6M/7M/8M bandwidths.
- Features H.264 MPEG-4 AVC video encoding at 1.000-18.000 Mbps and MPEG-1 Layer 2 audio at 48KHz.
- Accepts HDMI and CVBS inputs, handling resolutions up to 1080p/i.
- Provides adjustable RF output with 150-950MHz frequency range and -47 to 0 dBm level.
- Includes local LCD management and USB upgrade for system maintenance.
System Connection
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Technical Specifications
 
	HDMI Encoding Section

	Video
	Encoding
	H.264 MP@L 3.0/3.1/4.0

	
	Interface
	HDMI*1

	
	 
	Input
	Output

	
	Resolution
	480@59.94/60p
	480@60p

	
	
	480@59.94/60i
	480@30p

	
	
	576@50i
	576@25p

	
	
	720@50/59.94/60p
	720@50/59.94/60p

	
	
	1080@50i
	1080@25p

	
	
	1080@59.94/60i
	1080@30p

	
	
	1080@59.94/60p
	1080@30p

	
	Aspect Ratio
	16:9, 4:3

	
	Bit rate
	1.000~18.000 Mbps

	Audio
	Encoding
	MPEGI layer 2

	
	Sample rate
	48KHz

	 
	Bit rate
	64, 96,128, 192, 256, 320kbps

	CVBS Encoding Section

	Video
	Encoding
	H.264 MP@L 3.0

	
	Interface
	CVBS*1 (RCA)

	
	Resolution
	Input
	Output

	
	
	480@60p
	480@60p

	
	
	480@60i
	480@30p

	
	
	576@50p
	576@50p

	
	 
	576@50i
	576@25p

	
	Aspect Ratio
	4:3

	
	Bit rate
	1.000~18.000 Mbps

	Audio
	Encoding
	MPEGI layer 2

	
	Interface
	Analog Stereo/Mono (Unbalanced RCA)

	
	Sample rate
	48KHz

	
	Bit rate
	64, 96,128, 192, 256, 320kbps

	ISDB-T Modulator Section

	Standard
	ARIB STD-B31

	Bandwidth
	6M

	Constellation
	QPSK, 16QAM, 64QAM

	Guard Interval
	1/32, 1/16, 1/8, 1/4

	Transmission Mode
	2K, 4K, 8K

	MER
	≥30dB

	RF frequency
	150~950MHz, 0.1MHz step

	RF output level
	-47~ 0 dBm (60~107 dbµV), 1db step

	DVB-T Modulator Section

	Standard
	DVB-T COFDM

	Bandwidth
	6M, 7M, 8M

	Constellation
	QPSK, 16QAM, 64QAM

	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	Guard Interval
	1/32, 1/16, 1/8, 1/4

	Transmission Mode:
	2K, 8K

	MER
	≥31dB

	RF frequency
	150~950 MHz,0. 1KHz step

	RF output level
	-47~ 0 dBm (60~107 dbµV), 1db step

	System

	RF mix in ATT
	10 dB

	Management
	Local LCD + control buttons

	Language
	English

	Upgrade
	USB

	General

	Power supply
	DC 12V

	Dimensions
	183*110*50mm

	Weight
	< 1kg


 
 
Typical Applications
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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