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FMUSER FUQ-4635S HDMI Encoder Modulator 4 HDMI Inputs 2 RF DVB-C-T Outputs MPEG-4 AVC H.264 CATV Headend IPTV System  
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Product Overview
The FUQ-4635S/FUQ-4639S integrates MPEG-4 AVC/H.264 encoding and DVB-C/T modulation in a 1RU chassis, supporting 4/8 HDMI inputs, 64/128 IP streams, and 2/4 RF carriers. It processes signals with PID remapping and PSI/SI editing, delivering MPTS via Gigabit Ethernet. Controlled via web interface, this unit is designed for hotel TV systems, CATV headends, and multi-dwelling unit deployments. 
Key feature
 	Provides web-based control for configuration and monitoring
 
 
Principle Chart
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Technical Specification
	Input
	4/8 HDMI inputs;
64/128 IP inputs;
1 DVB-C/T/ISDB-Tb tuner input for re-mux (Optional for FU-4639S with DVB-C RF out version)

	Video
	Encoding
	MPEG-4 AVC/H.264

	
	Resolution
	In-put
	1920×1080_60P, 1920×1080_60i,
1920×1080_50P, 1920×1080_50i,
1280×720_60P, 1280×720_50P,
720×576_50i,720×480_60i,

	
	
	Out-put
	1920×1080_30P, 1920×1080_25P,
1280×720_30P, 1280×720_25P,
720×576_25P,720×480_30P,

	
	Bit-rate
	1Mbps~13Mbps each channel

	
	Rate Control
	CBR/VBR

	Audio
	Encoding
	MPEG-1 Layer 2, LC-AAC, HE-AAC and AC3 Pass Through

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 Adjustable

	
	MPEG-1 Layer 2 bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	LC-AAC bit-rate
	48/56/64/80/96/112/128/160/192/224/256/320/384 kbps

	
	HE-AAC bit-rate
	48/56/64/80/96/112/128 kbps

	Multiplexing
	Maximum PID
Remapping
	180 input per channel

	
	Function
	PID remapping ( automatically or manually)

	
	
	Generate PSI/ SI table automatically

	Scrambling
(optional for FU-4639S with DVB-C RF out version)
	Maximum simulcrypt CA
	4

	
	Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	DVB-C
	RF out
	2/4*RF DVB-C out (2/4 carriers combined output), F type interface

	
	
	Standard
	EN300 429/ITU-T J.83A/B

	
	
	MER
	≥40db

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF output level
	-25~-1dBm (82~105 dbµV), 0.1dBm

	
	
	Symbol Rate
	5.0Msps~7.0Msps, 1ksps stepping

	
	
	 
	J.83A
	J.83B

	
	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM

	
	
	Bandwidth
	8M
	6M

	
	DVB-T
	RF out
	2/4*RF COFDM DVB-T out (2/4 carriers combined output) ,F type interface

	
	
	Standard
	EN300744

	
	
	FFT mode
	2K,

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥42 dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF output level
	-28~ -3 dBm (77~97 dbµV), 0.1db step

	Stream output
	2/4 IP MPTS output over UDP/RTP/RTSP, 1*1000M Base-T Ethernet interface

	System function
	Network management(WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension (W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ±10%,50/60Hz


 
Order Guide
	 
	FU-4635S
	FU-4639S (DVB-C Out)
	FU-4639S (DVB-T Out)

	HDMI input
	4
	8
	8

	IP input
	64
	128
	128

	1 DVB-C/T/ISDB-Tb tuner input
	N/A
	Option as order
	N/A

	Scrambling function
	N/A
	Option as order
	N/A

	IP output
	2 MPTS
	4 MPTS
	4 MPTS

	DVB-C/T RF output channel
	2
	4
	4


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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