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Product Overview
The FMUSER FUQ-4637SB is a cost-effective encoder modulator with 16 CVBS inputs, 128 IP inputs, and 4ch DVB-C/T outputs. It performs MPEG4 AVC/H.264 encoding and multiplexing for signal processing. Controlled via web management, it supports real-time monitoring. Ideal for CATV broadcasting systems in next-gen deployments.
Key feature
Supports 16 CVBS inputs with MPEG4 AVC/H.264 encoding for robust video processing.  
Features 128 IP inputs over UDP/RTP for re-mux and 4MPTS IP output, plus optional ASI output.  
Provides 4ch DVB-C/T non-adjacent carrier outputs with multiplexing and optional scrambling.  
Includes audio encoding (MPEG1 Layer II) with gain adjustment and PSI/SI editing support.  
Offers web management for easy control, updates, and bit-rate monitoring. 
Principle Chart
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DVB-C RF output
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DVB-T RF output
 
Technical Specification
	Input
	16 CVBS inputs , DB15-To-RCA interface
128 IP (100/1000M)input over UDP and RTP protocol
1DVB-C tuner input for re-mux (optional)

	Video
	Resolution
	720×576i (PAL-B, D, G, H, I), 720×480i (NTSC-M, J)

	
	Encoding
	MPEG4 AVC/H.264(HP/MP/BP)

	
	Bit-rate
	1Mbps~5Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IPP (P frame is adjustable)

	Audio
	Encoding
	MPEG-1 Layer 2

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Audio Gain
	0-255 adjustable

	
	Bit-rate
	64/128/192/224/256/320/384Kbps each channel

	Modulation
	DVB-C
	4* DVB-C non-adjacent carriers 
Standard: EN300 429/ITU-T J.83A/B
MER: ≥40dB
RF frequency: 50~960MHz, 1KHz step
RF out level: -20~+3dBm (87~110 dBµV), 0.1dB step
Symbol Rate: 5.0Msps~7.0Msps, 1ksps step

	
	
	 
	J.83A
	J.83B

	
	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM

	
	
	Bandwidth
	8M
	6M

	
	DVB-T
	Standard
	EN300744

	
	
	FFT mode
	2K, 4K, 8K

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥40dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	4*COFDM DVB-T non-adjacent carriers

	
	
	RF out level
	-20~+3 dBm (87~110 dBµV), 0.1dB step

	Scrambling
(for DVB-C out version)
	Max simulscrypt CA
	4

	
	Scramble Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Stream output
	IP (4*MPTS) output as mirror of 4 carriers over UDP and RTP, 100/1000 Base-T Ethernet interface (Multicast/unicast)
1*ASI output (optional)

	System function
	Network management (WEB)

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×328mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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