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FMUSER FUQ-4653AB Multi-channel Encoder 8-24 CVBS Input to IP Output MPEG2-MPEG4 AVC-H264 Encoding Multiplexing Digital CATV Satellite Headend[image: 014]
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Product Overview
The FUQ-4653AB multi-channel encoder performs MPEG-2 and MPEG4 AVC/H.264 encoding and multiplexing. It converts 8/12/16/24 CVBS inputs into IP output streams. This unit offers optional ASI output and is managed via web interface. It provides cost-effective solutions for digital cable TV headends and satellite broadcasting systems. 
Key feature
Integrated MPEG-2 and MPEG4 AVC/H.264 video encoding. Supports 8/12/16/24 CVBS inputs with SPTS or MPTS output. Features MPEG1 Layer 2, LC-AAC, and HE-AAC audio encoding. Delivers IP output via UDP, RTP/RTSP + optional ASI copy. Provides management via web interface for control/updates.
Principle Chart
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Technical specification
	Input
	8/12/16/24 CVBS inputs , RCA interface

	Video
	Resolution
	Input
	Output

	
	
	720*576@50i
	720*576/352*288/320*240/320*180/
176*144/160*120/160*90@50Hz

	
	
	720*480@60i
	720*480/352*288/320*240/320*180/
176*144/160*120/160*90@60Hz

	
	Encoding
	MPEG-2, MPEG4 AVC/H.264

	
	Bit-rate
	0.5~5Mbps

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IPPP, IBPBP, IBBPB, IBBBP

	
	Advanced Pretreatment
	De-interlacing, noise reduction

	Audio
	Encoding
	MPEG1 Layer 2, LC-AAC, HE-AAC

	
	Sampling rate
	48KHz

	
	Bits per sample
	32-bit

	
	Bit-rate
	48Kbps~384Kbps (each channel)

	Multiplexing
	Function
	PID remapping (automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/ SI table automatically

	Stream output
	1 ASI out as copy of MPTS
IP output over UDP/RTP/RTSP through Data 1(1000M) or Data 2 (100M) :
8/12 CVBS inputs with 8/12 SPTS and 1 MPTS output
16/24 CVBS inputs with 16/24 SPTS or 1 MPTS output (alternative)

	System function
	Network management (WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×410mm×44mm

	
	Approx weight 
	8kg

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements 
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz

	
	Power consumption 
	20W


 
Order Information
	 
	FU-4653KB-8
	FU-4653KB-12
	FU-4653KB-16
	FU-4653KB-24

	8 CVBS Input
	                    √
	 
	 
	 

	12 CVBS Input
	 
	                    √
	 
	 

	16 CVBS Input
	 
	 
	                       √
	 

	24CVBS Input
	 
	 
	 
	                   √


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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