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Product Overview
The FUQ-4653B/FUQ-4653AB Encoder processes 8/12/24 CVBS inputs to deliver IP and ASI outputs with encoding and multiplexing. It converts signals by encoding video in MPEG-2 and audio in MPEG1 Layer II/AC3, supporting PAL/NTSC formats. Control is via web-based management for configuration and updates. Ideal for digital head-end systems in broadcasting and cable TV applications. 
Key feature
For FUQ-4653AB: Adds QR Code, Caption, and Logo insertion capabilities 
Principle Chart
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Technical specification
	Input
	8/12/24CVBS inputs , RCA interface

	Video
	Resolution
	720×480_60i, 544×480_60i, 352×480_60i
352×240_60i, 320×240_60i,176×240_60i, 176×120_60i

	
	
	720×576_50i, 704×576_50i, 640×576_50i, 352×288_50i, 320×288_50i, 176×288_50i, 176×144_50i

	
	Encoding
	MPEG-2

	
	Bit-rate
	0.5Mbps~8Mbps each channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	GOP_0_B, GOP_1_B, GOP_2_B, GOP_3_B

	
	Advanced Pretreatment
	De-interlacing, noise reduction

	Audio
	Encoding
	MPEG-1 Layer 2, AC3(2.0)

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Bit-rate
	64Kbps,128Kbps,192kbps,256kbps,320kbps,384kbps each channel

	Multiplexing
	Function
	PID remapping (automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/ SI table automatically

	Stream output
	1 ASI as copy of MPTS
IP (MPTS/SPTS) output over UDP/RTP/RTSP
8/12 CVBS inputs with 8/12 SPTS and 1 MPTS output
24×CVBS inputs with 24 SPTS or 1 MPTS output

	System function
	Network management (WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension(W×L×H)
	482mm×410mm×44mm

	
	Approx weight 
	8kg

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements 
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz

	
	Power consumption 
	20W


 
Order Information
	 
	FU-4653K/KA-8
	FU-4653K/KA-12
	FU-4653K/KA-24

	8CVBS Input
	                      √
	 
	 

	12CVBS Input
	 
	                    √
	 

	24CVBS Input
	 
	 
	                     √


  


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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