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The FUQ-4655XY is a high-integration encoder modulator combining encoding, multiplexing, scrambling, and modulation. It features 12 HD-SDI inputs, a DVB-C tuner, and up to 512 IP inputs via Data1 port, with DVB-C RF output supporting 16 carriers. Optional outputs include DVB-T, ATSC, or ISDB-T RF with fewer carriers and ASI mirroring. This device is ideal for broadcast studios, cable headends, and professional video distribution systems. 
Key feature
Includes optional ASI output and web-based management for remote control.
 
Principle Chart
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DVB-C Principle Chart
[image: IMG_257]
DVB-T/ATSC Principle Chart
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ISDB-T Principle Chart
 
Technical specification
	Input
	12 HD-SDI inputs with CC
1 DVB-C (ATSC optional)Tuner for re-mux, F type interface
512 IP input over UDP and RTP, DATA1, RJ45—DVB-C RF out
256 IP input over UDP and RTP, DATA1, RJ45—DVB-T/ATSC RF out
192 IP input over UDP and RTP, DATA1, RJ45—ISDB RF out

	Video
	Resolution
	Input
	1920*1080_60p, 1920*1080_50p,1920*1080_60i, 1920*1080_50i, 1280*720_60p, 1280*720_50P,
720*480_60i, 720*576_50i

	
	
	Output
	1920*1080_60p, 1920*1080_50p,1920*1080_60i, 1920*1080_50i, 1440*1080_60i, 1440*1080_50i,
1280*720_60p, 1280*720_50P, 720*576_50p,
720*576_50i, 720*576_30p, 720*576_25p,
720*480_60p, 720*480_60i,720*480_30p, 720*480_25p,320*240_60p,320*240_50p,
320*240_30p, 320*240_25p,320*180_60p, 320*180_50p, 320*180_30p, 320*180_25p,
960*540_50i, 704*576_50i,704*480_60i, 640*576_50i
640*480_60i, 544*576_50i,544*480_60i,

	
	Encoding
	MPEG2 & MPEG4 AVC/H.264

	
	Bit-rate
	0.8~19Mbps for H.264 encoding
1~19Mbps for MPEG-2 encoding

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	GOP B Frame: 0-3, GOP P Frame: 0-6

	
	Advanced Pretreatment
	De-interlacing, noise reduction

	Audio
	Encoding
	MPEG1 Layer II, MPEG2-AAC, MPEG4-AAC,
Dolby Digital AC3 (2.0) encoding (Optional),
AC3 (2.0/5.1) passthrough

	
	Sampling rate
	48KHz

	
	Bit-rate
	64Kbps-320kbps each channel

	Multiplexing
	Maximum PID
Remapping
	256 input per channel

	
	Function
	PID remapping ( automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/ SI table automatically

	Scrambling
	Maximum simulcrypt CA
	4

	
	Standard
	ETR289, ETSI 101197, ETSI 103197

	
	Connection
	Local/remote connection

	Modulation
	DVB-C
	QAM Channel: 16 non-adjacent carriers output (maximum bandwidth 192MHz)
Standard: EN300 429/ITU-T J.83A/B
MER: ≥40db
RF frequency: 50~960MHz, 1KHz step
RF output level: -20~+10dbm, 0.1db step
Symbol Rate: 5.0Msps~7.0Msps, 1ksps stepping

	
	
	 
	J.83A
	J.83B

	
	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM

	
	
	Bandwidth
	8M
	6M

	
	DVB-T
	Standard
	EN300744

	
	
	FFT mode
	2K, 4K, 8K

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥42 dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	8 non-adjacent carriers output (maximum bandwidth 192MHz)

	
	
	RF output level
	-20~+10 dBm, 0.1db step

	
	ATSC
	Standard
	ATSC A/53

	
	
	Bandwidth
	6M

	
	
	Constellation
	8VSB

	
	
	FEC
	RS(208 188)+Trellis

	
	
	MER
	≥40dB

	
	
	ACL
	-55 dBc

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	8 non-adjacent carriers output (maximum bandwidth 192MHz)

	
	
	RF output level
	-20~+10dbm (for all carriers), 0.5db stepping

	
	ISDB-T
	Standard
	ARIB STD-B31

	
	
	Bandwidth
	6M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/32, 1/16, 1/8, 1/4

	
	
	Transmission Mode
	2K, 4K, 8K

	
	
	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥40dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	6 non-adjacent carriers output (maximum bandwidth 192MHz)

	
	
	RF output level
	-20dBm~+10dBm, 0.1dB stepping

	Stream output
	1 ASI output as mirror of one of RF output carriers-Optional
16 MPTS output over UDP and RTP/RTSP as mirror of 16 DVB-C carriers,
8 MPTS output over UDP and RTP/RTSP as mirror of 8 DVB-T/ATSC carriers(Optional)
6 MPTS output over UDP and RTP/RTSP as mirror of 6 ISDB-T carriers(Optional)
1*1000M Base-T Ethernet interface

	System function
	Network management (WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension (W×L×H)
	482mm×440mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
Ordering Information
	 
	IP input
	IP output
	RF carriers
	Scrambling

	DVB-C
	512
	16
	16
	√

	DVB-T
	256
	8
	8
	×

	ATSC
	256
	8
	8
	×

	ISDB-T
	192
	6
	6
	×


                                              

 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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