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The FUQ-4655AB encoder processes signals with 12 HD-SDI inputs and 32 IP inputs, outputting 1 MPTS and 12 SPTS over UDP/RTP/RTSP. It encodes video in MPEG-2 or MPEG-4 AVC/H.264 and handles Dolby Digital AC3 audio. Managed via a web interface, this unit is optimized for CATV, satellite, and terrestrial digital TV systems.
Key feature
Supports 12 HD-SDI inputs for MPEG-2 or MPEG-4 AVC/H.264 encoding with EIA608/EIA708 closed captioning.  
Handles audio encoding including MPEG1 Layer II, MPEG2-AAC, MPEG4-AAC, and Dolby Digital AC3 (2.0) with passthrough.  
Provides 32 IP inputs over UDP/RTP and outputs 1 MPTS/12 SPTS via DATA1/DATA2 ports.  
Enables PID remapping, PCR adjusting, and PSI/SI table editing/inserting.  
Features web-based management for configuration and updates.
Principle Chart
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Technical Specification
 
	Input
	12 HD-SDI inputs with CC (EIA608/EIA708)
32 IP input over UDP and RTP through DATA 1 port

	Video
	Resolution
	Input
	1920*1080_60p, 1920*1080_50p,1920*1080_60i, 1920*1080_50i, 1280*720_60p, 1280*720_50P,
720*480_60i, 720*576_50i

	
	
	Output
	1920*1080_60p, 1920*1080_50p,1920*1080_60i, 1920*1080_50i, 1440*1080_60i, 1440*1080_50i,
1280*720_60p, 1280*720_50P, 720*576_50p,
720*576_50i, 720*576_30p, 720*576_25p,
720*480_60p, 720*480_60i,720*480_30p, 720*480_25p,320*240_60p,320*240_50p,
320*240_30p, 320*240_25p,320*180_60p, 320*180_50p, 320*180_30p, 320*180_25p,
960*540_50i, 704*576_50i,704*480_60i, 640*576_50i
640*480_60i, 544*576_50i,544*480_60i,

	
	Encoding
	MPEG2 & MPEG4 AVC/H.264

	
	Bit-rate
	0.8~19Mbps for H.264 encoding
1~19Mbps for MPEG-2 encoding

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	GOP B Frame: 0-3, GOP P Frame: 0-6

	Audio
	Encoding
	MPEG1 Layer II, MPEG2-AAC, MPEG4-AAC,
Dolby Digital AC3 (2.0) encoding,
AC3 (2.0/5.1) passthrough

	
	Sampling rate
	48KHz

	
	Bit-rate
	64Kbps-320kbps each channel

	Multiplexing
	Maximum PID
Remapping
	180 input per channel

	
	Function
	PID remapping ( automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/ SI table automatically

	Stream output
	1 MPTS and 12 SPTS IP output over UDP and RTP/RTSP, 2*1000M Base-T Ethernet interface, Data 1 and Data 2
1 ASI output as mirror of MPTS-Optional

	System function
	Network management (WEB)

	
	Ethernet software upgrade

	Miscellaneous
	Dimension (W×L×H)
	482mm×440mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 
                                               


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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