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FMUSER FUQ-4655BC Encoder Modulator 24 CVBS & 512 IP Inputs 16 RF Outputs MPEG-2 Encoding DVB-C-DVB-T-ATSC-ISDB-T Multiplexing Scrambling CATV Headend Hotel TV System
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Product Overview
The FMUSER FUQ-4655BC is a professional SD encoder modulator integrating encoding, multiplexing, scrambling, and modulation, with 24 CVBS inputs and IP streaming via the DATA1 port. It processes signals using MPEG-2 video encoding and MPEG-1 Layer 2 or DD AC3 audio encoding, outputting DVB-C, DVB-T/ATSC, or ISDB-T signals. Featuring web-based management for control and updates, it is ideal for small CATV headends and broadcast systems, enabling efficient signal distribution. 
Key feature
Comprehensive multiplexing with PID remapping, PCR adjusting, and PSI/SI editing. 
Principle Chart
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DVB-C Principle Chart
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DVB-T Principle Chart
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ISDB-T Principle Chart
 
Technical specification
	Input
	24 CVBS inputs
1 DVB-C(ATSC optional) Tuner for re-mux, F type interface
512 IP input over UDP and RTP, DATA1, RJ45—DVB-C RF out
256 IP input over UDP and RTP, DATA1, RJ45—DVB-T/ATSC RF out
192 IP input over UDP and RTP, DATA1, RJ45—ISDB RF out

	Video
	Resolution
	720×480_60i, 544×480_60i, 352×480_60i
352×240_60i,320×240_60i,176×240_60i, 176×120_60i

	
	
	720×576_50i,704×576_50i,640×576_50i, 352×288_50i
320×288_50i, 176×288_50i, 176×144_50i

	
	Encoding
	MPEG-2

	
	Bit-rate
	0.5Mbps~8Mbps per channel

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP, IBP, IBBP, IBBBP

	
	Advanced Pretreatment
	De-interlacing, noise reduction

	Audio
	Encoding
	MPEG-1 Layer 2, DD AC3 (2.0)

	
	Sampling rate
	48KHz

	
	Resolution
	24-bit

	
	Bit-rate
	64Kbps,128Kbps,192kbps,256kbps,320kbps,384kbps each channel

	Multiplexing
	Maximum PID
Remapping
	180 input per channel

	
	Function
	PID remapping ( automatically or manually)

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/ SI table automatically

	Scrambling
	Maximum simulcrypt CA
	4

	
	Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/remote connection

	Modulation
	 
 
 
DVB-C
 
 
 
	QAM Channel
	16 non-adjacent carriers output (maximum bandwidth

	
	
	Standard
	EN300 429/ITU-T J.83A/B

	
	
	MER
	≥40db

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF output level
	-20~+10dbm (87~107 dbµV), 0.1db step

	
	
	Symbol Rate
	5.0Msps~7.0Msps, 1ksps stepping

	
	
	 
	J.83A
	J.83B

	
	
	Constellation
	16/32/64/128/256QAM
	64/256 QAM

	
	
	Bandwidth
	8M
	6M

	
	DVB-T
	Standard
	EN300744

	
	
	FFT mode
	2K,4K, 8K

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥42 dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	8 non-adjacent carriers DVB-T out (maximum bandwidth 192MHz)

	
	
	RF output level
	-20~ +10 dBm (77~97 dbµV), 0.1db step

	
	ATSC
	Standard
	ATSC A/53

	
	
	Bandwidth
	6M

	
	
	Constellation
	8VSB

	
	
	FEC
	RS(208 188)+Trellis

	
	
	MER
	≥40dB

	
	
	ACL
	-55 dBc

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	8 non-adjacent carriers output (maximum bandwidth 192MHz)

	
	
	RF output level
	-20~+10dbm (for all carriers), 0.5db stepping

	
	ISDB-T
	Standard
	ARIB STD-B31

	
	
	Bandwidth
	6M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/32, 1/16, 1/8, 1/4

	
	
	Transmission Mode
	2K, 4K, 8K

	
	
	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥40dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	6 non-adjacent carriers output (maximum bandwidth 192MHz)

	
	
	RF output level
	-20dBm~+10dBm, 0.1dB stepping

	Stream output
	1 ASI output as mirror of one of RF output carriers-Optional
16 MPTS output over UDP and RTP/RTSP as mirror of 16 DVB-C carriers,
8 MPTS output over UDP and RTP/RTSP as mirror of 8 DVB-T/ATSC carriers(Optional)
6 MPTS output over UDP and RTP/RTSP as mirror of 6 ISDB-T carriers(Optional)
1*1000M Base-T Ethernet interface

	System function
	Network management (WEB)

	
	Chinese and English language

	
	Ethernet software upgrade

	Miscellaneous
	Dimension (W×L×H)
	482mm×440mm×44mm

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	AC 110V± 10%, 50/60Hz, AC 220 ± 10%, 50/60Hz


 

 
Ordering Information
	 
	IP input
	IP output
	RF carriers
	Scrambling

	DVB-C
	512
	16
	16
	√

	DVB-T
	256
	8
	8
	×

	ATSC
	256
	8
	8
	×

	ISDB-T
	192
	6
	6
	×


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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