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FMUSER FUQ-46610F IP Gateway 16 Tuner Inputs 2 ASI Inputs DVB-S-S2-S2X DVB-C-T ATSC ISDB-T to 512 SPTS 16 MPTS IP Outputs BISS Descrambling Web Management Broadcast Headend [image: 3EEECN_20171201035820]
 
Product overview
The FUQ-46610F is a professional IP gateway converting 16 tuner inputs (supporting DVB-S/S2/S2X, DVB-C/T, ATSC, or ISDB-T) or 2 ASI feeds into IP streams. It processes signals into 512 SPTS (PID-filtered) or 16 MPTS (Null PKT filtered) outputs via dual Gigabit Ethernet ports with BISS descrambling. The 1RU rack-mount unit features web-based control and DiSEqC switching. Ideal for broadcast headend digitization, IPTV distribution, and multi-standard signal aggregation in terrestrial/satellite systems. 
Key feature
 Web-based management for remote signal monitoring and control 
Working Principle
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Specifications
	Input
	Optional 1:16 tuners input +2 ASI input---SPTS output
Optional 2:14 tuners input +2 ASI input --- MPTS output
Optional 3:16 tuners input --- MPTS output

	Tuner Section
	Multi-mode tuners switchable
(New Type)
	DVB-C
	Frequency In
	60~890MHz

	
	
	
	Standard
	J.83A(DVB-C), J.83B, J.83C

	
	
	
	Constellation
	16/32/64/128/256 QAM

	
	
	DVB-T/(T)
	Frequency In
	60~890MHz

	
	
	
	Bandwidth
	6/7/8 M bandwidth

	
	
	ISDB-T
	Frequency In
	60~890MHz

	
	Version 1
	DVB-S
	Frequency In
	950-2150MHz

	
	
	
	Symbol rate
	1~45 Msps

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	DVB-S2
	Frequency In
	950-2150MHz

	
	
	
	Symbol rate
	1~45 Msps

	
	
	
	FEC
	1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK

	
	Version 2
(New Type)
	DVB-S
	Frequency In
	950~2150MHz

	
	
	
	Symbol rate
	0.5~45Msps

	
	
	
	Signal Strength
	- 65- -25dBm

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	
	Max input bitrate
	≤125 Mbps

	
	
	DVB-S2
	Frequency In
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~34Msps;

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                           
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10                                           
 16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                          
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤125 Mbps

	
	
	DVB-S2X
	Frequency In
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~34Msps

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10, 2/3-L, 32/45, 11/15, 7/9

	
	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤125 Mbps

	
	 
	ATSC
	Frequency In
	54~858MHz

	
	
	
	Bandwidth
	6M bandwidth

	
	
	
	Constellation
	8VSB

	BISS Descrambling
	Mode 1, Mode E (Up to 850Mbps) (descramble individual program)

	Output
	512 SPTS IP mirrored output over UDP and RTP/RTSP protocol through GE1 and GE2 port (IP address and port number of GE1 and GE2 are different) , Unicast and Multicast

	
	16 MPTS IP output (for Tuner/ASI passthrough) over UDP and RTP/RTSP protocol through GE1 and GE2 port, Unicast and Multicast

	System
	Web based management

	
	Ethernet software upgrade

	Miscellaneous
	Dimension
	482mm×410mm×44mm (W×L×H)

	
	Approx weight 
	3.6kg

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements 
	100~240VAC, 50/60Hz

	
	Power consumption 
	20W
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Tuner Input Options:
	· 8 DVB-C Tuners + 8 ATSC Tuners

	· 8 DVB-C Tuners + 8 DVB-T/(T) Tuners

	· 8 DVB-S2/S2X Tuners + 8 DVB-T/(T) Tuners

	· 8 DVB-S2/S2X Tuners + 8 ISDB-T Tuners

	· 16 DVB-S/S2/S2X/DVB-C/T/(T) /ISDB-T/ATSC Tuners


 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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