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Product overview
The FUQ-4667XX is a professional encoder modulator featuring 1x HDMI input and dual RF/IP outputs. It processes 1080p60 signals via H.265/HEVC or H.264 encoding, then modulates to DVB-C/T, ATSC, or ISDB-T standards. This 1RU rack-mount device supports web-GUI and front-panel control. Ideal for cable TV headends, hospitality TV systems, and digital signage networks requiring multi-format distribution. 
Key feature
Remote management via web-GUI with AC3 audio pass-through support 
System Connection
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Appearance and Description

 
Technical Specs
 
	HDMI Encoding Section

	Video
	Encoding
	HEVC/ H.265 , MPEG 4 AVC/H.264

	
	Interface
	HDMI*1. HDMI loop out*1

	
	Resolution
	1920*1080_60P,
1920*1080_50P;
1920*1080_59.94P,
1280*720_60p,
1280*720_59.94
1280*720_50P

	
	Chroma
	4:2:0

	
	Bitrate
	1Mbps~15Mbps

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IP

	Audio
	Encoding Format
	MPEG-1 Layer 2,
LC-AAC, HE-AAC, HE-AAC V2;
AC3 Pass-through

	
	Sample rate
	32KHz,44.1KHz,48KHz

	
	Bit-rate
	48~384Kbps


 
	IP output

	IP out over UDP (Unicast/multicast), RTP/RTSP, (RJ45, 100M)

	DVB-C Modulator Section

	Standard
	J.83A (DVB-C), J.83B

	MER
	≥40dB

	RF frequency
	100-1000MHz, 1KHz step

	RF output level
	-20~ -5dBm, 1dB step

	Symbol rate
	5.000~7.000Msps adjustable

	 
	J.83A
	J.83B

	Constellation
	16/32/64/128/ 256 QAM
	64/ 256 QAM

	Bandwidth
	8M
	6M

	DVB-T Modulator Section

	Standard
	DVB-T COFDM

	Bandwidth
	6M, 7M, 8M 

	Constellation
	QPSK, 16QAM, 64QAM

	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	Guard Interval
	1/32, 1/16, 1/8, 1/4

	Transmission Mode:
	2K, 8K

	MER
	≥35dB

	RF frequency
	100-900MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	ISDB-T Modulator Section (Optional)

	Standard
	ARIB STD-B31

	Constellation   
	QPSK, 16QAM, 64QAM

	Guard Interval
	1/32, 1/16, 1/8, 1/4

	Transmission Mode
	2K, 4K, 8K

	Code rate
	1/2, 2/3, 3/4, 5/6, 7/8

	RF frequency
	100~900MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	ATSC Modulator Section (Optional)

	Standard
	ATSC A/53

	Constellation
	8 VSB

	RF output level
	-63~-16dBm (44~91 dBµV), 1dB step

	MER
	≥35dB

	RF frequency
	100~900MHz, 1KHz step

	RF output level
	-63~ -16dBm, 1dB step

	System

	Management
	Web-GUI, LED+Keyboard

	Language
	English

	Upgrade
	Web update

	General

	Power supply
	DC 12V

	Dimensions
	160*120*52mm

	Weight
	< 1kg


 
OSD (Logo/QR Code/Caption) Insertion
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Typical Applications
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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- Home Version

A device that allows audio and video signal input in TV distributions with applications

in home entertainment, Digital Signage for hotels, shops, restaurants etc...

Support CC (Closed Caption) /Teletext
Support Audio delay function

Teletext Standard as per EN300706 & EN300472
‘This NDS3556HS Encoder Modulator can support
Teletext function to pushing text information such as

domestic news, international news, sports news,

weather forecasts, TV program forccasts information

and subtitle etc.




image5.jpeg
CVBS out with
CC/Teletext

HDMI out 9 " ’
Video Distribution Network

with CC/Teletext
IP out .





image6.png
- RF for mix
€V

L
-

Monitor

Attenuation: 10dB

RF out TV+AV to the
distribution network

HDMI Input
Audio out

Lo,

Radio Broadcast
input

1P out
UDP, RTP/RTSP

Microphone




image8.png
LOGO Insertion
["® Support jpg/jpeg/bmp/gif/png file
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Caption Insertion
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for communities of residents ...for restaurants
an information channel on their television information about daily menus ,special deals etc

for hotels ...for hopitals
meeting rooms exhibitions, message. etc training cours

s, healthy guide, etc

.for Public Spaces ..for shopping centres
adversing user information news etc new collections,special deals etc
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