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FMUSER FUQ-467B Series SD IRD Dual RF-ASI-IP Inputs 2 ASI-IP-CVBS Outputs DVB-C DVB-T-T ISDB-T DVB-S-S2-S2X Demodulation Descrambling Decoding Broadcast Reception [image: 3EEECN_20180131053203]Its production is stopped temporarily, and the date for resuming production is not fixed yet.
 
Demodulation Module = 2*RF/Loop out + 2*CAM + 2*Smartcard
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Product overview
The FMUSER FUQ-467Y Series SD IRD integrates demodulation, descrambling, and decoding in a 1U chassis, with dual tuner inputs for RF, ASI, and IP sources. It processes signals by converting RF inputs to CVBS output, supporting standards like DVB-S/S2/S2X. The pluggable module design enables component customization. Ideal for broadcast distribution and television signal transmission.
Key feature
Integrated demodulation, descrambling, and decoding in one unit.  
Supports dual tuner inputs with DVB-S/S2/S2X, DVB-C, DVB-T/(T), and ISDB-T.  
Features BISS and CAM/CI descrambling for encrypted content.  
Pluggable modules for easy replacement of demodulator and decoder components.  
Delivers CVBS, ASI, and IP (UDP/RTP/RTSP) outputs.  
Principle Chart
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Technical Specifications
 
	Input
	2 *Tuner(DVB-C, T/(T), ISDBT, S/S2/S2X optional), F type
1*ASI input for re-mux, BNC interface
1*IP input for re-mux (UDP)
	 

	Tuner Section
	Multi-mode tuners switchable
(New)
	DVB-C
	Input Frequency
	60 ~890 MHz
	 

	
	
	
	Standard
	J.83A, J.83C
	J.83B
	 

	
	
	
	Constellation
	16/32/64/128/256 QAM
	64/256 QAM
	 

	
	
	DVB-T/(T)
	Input Frequency
	60 ~890 MHz
	 

	
	
	
	Bandwidth
	6/7/8 M
	 

	
	
	ISDB-T
	Input Frequency
	60 ~890 MHz
	 

	
	Version 1
	DVB-S
	Input Frequency
	950~2150MHz
	 

	
	
	
	Symbol rate
	1~45 Msps
	 

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8
	 

	
	
	
	Constellation
	QPSK
	 

	
	
	
	Signal Strength
	- 65~-25dBm
	 

	
	
	
	Max input bitrate
	≤120 Mbps
	 

	
	
	DVB-S2
	Input Frequency
	950~2150MHz
	 

	
	
	
	Symbol rate
	1~45 Msps
	 

	
	
	
	FEC
	1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
	 

	
	
	
	Constellation
	QPSK, 8PSK
	 

	
	
	
	Max input bitrate
	≤120 Mbps
	 

	
	Version 2
(New)
	DVB-S
	Input Frequency
	950~2150MHz
	 

	
	
	
	Symbol rate
	0.5~45Msps
	 

	
	
	
	Signal Strength
	- 65- -25dBm
	 

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8
	 

	
	
	
	Constellation
	QPSK
	 

	
	
	
	Max input bitrate
	≤160 Mbps
	 

	
	
	DVB-S2
	Input Frequency
	950~2150MHz
	 

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~40Msps;
	 

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                           
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10                                            
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                          
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10
	 

	
	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK
	 

	
	
	
	Max input bitrate
	≤160 Mbps
	 

	
	
	DVB-S2X
	Input Frequency
	950~2150MHz
	 

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~40Msps
	 

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9
	 

	
	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK
	 

	
	
	
	Max input bitrate
	≤160 Mbps
	 

	Descrambling
	CAM/CI Quantity
	2
	 

	
	BISS Mode
	Mode 1, Mode E (up to 120Mbps)
	 

	Output
	IP (1*MPTS & 8*SPTS) out over UDP, RTP/RTSP.
100Base-T Ethernet interface (unicast / multicast)
	 

	
	2×ASI mirrored out, BNC interface
	 

	
	2*CVBS optional
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	Decode Out
	Video Interface: 2xCVBS (RCA)
Audio Interface: 2xStereo/4xMono (RCA)
Resolution: PAL 576i, NTSC 480i
Video Decode: MPEG-2, MPEG-4 AVC/H.264(optional)
Audio Decode: MPEG 1 Layer II
	 

	
	4*CVBS optional
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	Decode Out
	Video Interface: 4xCVBS (RCA)
Audio Interface: 4xStereo/8xMono (RCA)
Resolution: PAL 576i, NTSC 480i
Video Decode: MPEG-2, MPEG-4 AVC/H.264
Audio Decode: MPEG 1 Layer II
	 

	System
	Local interface
	LCD + control buttons

	
	Remote management
	Web-server Management

	
	Language
	English

	
	Upgrade
	USB, web management

	Miscellaneous
	Dimension
	482*300*44.5mm  (W×L×H)
	 

	
	Approx weight 
	3.5kg
	 

	
	Environment
	0~45℃(work)；-20~80℃（Storage）
	 

	
	Power requirements 
	100~240VAC, 50/60Hz
	 

	
	Power consumption 
	20W
	 


 
 
 
 
 
 
 
System Connection Sample
 
[bookmark: _GoBack][image: IMG_260]
 
Ordering Guide 
	FU-467X, ‘X’ should be interpreted as different digits which indicate tuners of different standard.
* FU-4671 DVB-C SD IRD
*  FU-4674 DVB-(T) SD IRD
* FU-4675 DVB-S/S2 SD IRD
Multiple decoding boards are optional:
Option 1: 2 A/V output (MPEG-2 Decoding)- FU-467X
Option 2: 2 A/V output (MPEG-2 & MPEG-4 Decoding) – FU-467X-A
Option 3: 4 A/V output (MPEG-2 & MPEG-4 Decoding) – FU-467X-C


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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