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Product Overview
The FMUSER FUQ-4696 CI Receiver integrates demodulation and descrambling in a 1U chassis, supporting 2 or 4 tuner inputs and outputs via ASI or IP. It converts RF signals to TS output after re-mux, with CAM/CI decryption and web NMS management. Designed for broadcast systems, cable headends, and IPTV distribution.
 
Key feature
Supports 2 or 4 tuner inputs with switchable DVB-C/T/ISDB-T or optional DVB-S/S2/S2X/ATSC.
Features 1 ASI & 16 IP inputs for re-mux with UDP/RTP and BISS descrambling.
Includes CAM/CI slots for decrypting programs from RF, ASI, or IP without external power.
Provides output flexibility: 1 MPTS via ASI/IP and 16 SPTS over IP (UDP/RTP).
Offers web NMS management with remote control, firmware updates, and 256 PID mapping. 
 
Principle Chart (each demodulation module)
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Technical Specifications
	Input(per demodulation module)
	2 or 4* tuner inputs (DVB-C/T/ISDB-T switchable or DVB-S/S2/S2X or ATSC optional), F type
1*ASI input for re-mux, BNC interface
16*IP input for re-mux (UDP/RTP)

	 Tuner Section
	Multi-mode tuners switchable
(New)
	DVB-C
	Input Frequency
	60 ~890 MHz

	
	
	
	Standard
	J.83A, J.83C
	J.83B

	
	
	
	Constellation
	16/32/64/128/256 QAM
	64/256 QAM

	
	
	DVB-T
	Input Frequency
	60 ~890 MHz

	
	
	
	Bandwidth
	6/7/8 M

	
	
	ISDB-T
	Input Frequency
	60 ~890 MHz

	
	Satellite
	DVB-S
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	0.5~45Msps

	
	
	
	Signal Strength
	- 65- -25dBm

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	
	Max input bitrate
	≤170 Mbps

	
	
	DVB-S2
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~40Msps;

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                           
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10                                            
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                          
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤170 Mbps

	
	
	DVB-S2X
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~40Msps

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤170 Mbps

	 
	ATSC
	ATSC
	Input Frequency
	54-858MHz

	
	
	
	Bandwidth
	6 M

	
	
	
	Constellation
	8 VSB

	Descrambling
	CAM/CI Quantity
	2 (per demodulation module)

	
	BISS Mode
	Mode 1, Mode E

	Output (per demodulation module)
	1*MPTS & 16*SPTS over UDP, RTP.
1000 Base-T Ethernet interface (unicast / multicast)

	
	1×ASI mirrored out of MPTS, BNC interface

	System
	Remote management
	Web-server Management

	
	Language
	English

	
	Upgrade
	web management

	Miscellaneous
	Dimension
	482*300*44mm (W×L×H)

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	100~240VAC, 50/60Hz

	
	Power consumption 
	15W


 
 
 
Order Guide
Please specify both Demodulation module and Tuner Input options when you place order:
 
	Demodulation Module
	Option 1
	1*Demodulation module, 2 CAM/CI Slots

	
	Option 2
	2*Demodulation modules, 4 CAM/CI Slots


 
	Tuner Input  (per demodulation module)
	Option 1
	2*DVB-S/S2/S2X tuner

	
	Option 2
	2*DVB-C/T/ISDB-T tuner

	
	Option 3
	2*ATSC tuner

	
	Option 4
	4*DVB-S/S2/S2X tuner

	
	Option 5
	4*DVB-C/T/ISDB-T tuner

	
	Option 6
	4*ATSC tuner

	
	Option 7
	2*DVB-S/S2/S2X tuner + 2*DVB-C/T/ISDB-T tuner

	
	Option 8
	2*DVB-S/S2/S2X tuner + 2* ATSC tuner

	
	Option 9
	2*DVB-C/T/ISDB-T tuner + 2*ATSC tuner


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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