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Product overview 
The FUQ-4696 is a CI receiver integrating demodulation and descrambling, with inputs including 2/4 tuners for RF signals, 1 ASI input, and 16 IP inputs, and outputs such as 1 ASI output and IP TS streams ( 1 MPTS and 16 SPTS). It processes signals by demodulating inputs, descrambling encrypted content using CAM/CI slots and BISS, and re-muxing into transport streams. This 1-U rack-mountable device supports web-based management. Ideal for broadcast headend applications like content distribution and signal processing.
 
Key feature
Supports multi-standard tuner inputs for DVB-C/T/ISDB-T, DVB-S/S2/S2X, ATSC with 2/4 tuners,  
Features re-mux flexibility with 1 ASI input and 16 IP inputs (UDP/RTP),  
Provides decryption via 2 CAM/CI slots and BISS descrambling,  
Offers versatile outputs including 1 MPTS, 16 SPTS over IP, and ASI output,  
Enables web-based management for remote control and updates.
 
Principle Chart (each demodulation module)
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Technical Specifications
	Input(per demodulation module)
	2 or 4* tuner inputs (DVB-C/T/ISDB-T switchable or DVB-S/S2/S2X or ATSC optional), F type
1*ASI input for re-mux, BNC interface
16*IP input for re-mux (UDP/RTP)

	 Tuner Section
	Multi-mode tuners switchable
(New)
	DVB-C
	Input Frequency
	60 ~890 MHz

	
	
	
	Standard
	J.83A, J.83C
	J.83B

	
	
	
	Constellation
	16/32/64/128/256 QAM
	64/256 QAM

	
	
	DVB-T
	Input Frequency
	60 ~890 MHz

	
	
	
	Bandwidth
	6/7/8 M

	
	
	ISDB-T
	Input Frequency
	60 ~890 MHz

	
	Satellite
	DVB-S
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	0.5~45Msps

	
	
	
	Signal Strength
	- 65- -25dBm

	
	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	
	Constellation
	QPSK

	
	
	
	Max input bitrate
	≤170 Mbps

	
	
	DVB-S2
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
32APSK: 0.5~40Msps;

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                           
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10                                            
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10                                          
32APSK: 3/4, 4/5, 5/6, 8/9, 9/10

	
	
	
	Constellation
	QPSK, 8PSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤170 Mbps

	
	
	DVB-S2X
	Input Frequency
	950~2150MHz

	
	
	
	Symbol rate
	QPSK/8PSK /16APSK :0.5~45 Msps
8APSK: 0.5~40Msps
32APSK: 0.5~40Msps

	
	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36 , 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	
	Constellation
	QPSK, 8PSK, 8APSK, 16APSK, 32APSK

	
	
	
	Max input bitrate
	≤170 Mbps

	 
	ATSC
	ATSC
	Input Frequency
	54-858MHz

	
	
	
	Bandwidth
	6 M

	
	
	
	Constellation
	8 VSB

	Descrambling
	CAM/CI Quantity
	2 (per demodulation module)

	
	BISS Mode
	Mode 1, Mode E

	Output (per demodulation module)
	1*MPTS & 16*SPTS over UDP, RTP.
1000 Base-T Ethernet interface (unicast / multicast)

	
	1×ASI mirrored out of MPTS, BNC interface

	System
	Remote management
	Web-server Management

	
	Language
	English

	
	Upgrade
	web management

	Miscellaneous
	Dimension
	482*300*44mm (W×L×H)

	
	Environment
	0~45℃(work)；-20~80℃（Storage）

	
	Power requirements  
	100~240VAC, 50/60Hz

	
	Power consumption 
	15W


 
 
 
Order Guide
Please specify both Demodulation module and Tuner Input options when you place order:
 
	Demodulation Module
	Option 1
	1*Demodulation module, 2 CAM/CI Slots

	
	Option 2
	2*Demodulation modules, 4 CAM/CI Slots


 
	Tuner Input  (per demodulation module)
	Option 1
	2*DVB-S/S2/S2X tuner

	
	Option 2
	2*DVB-C/T/ISDB-T tuner

	
	Option 3
	2*ATSC tuner

	
	Option 4
	4*DVB-S/S2/S2X tuner

	
	Option 5
	4*DVB-C/T/ISDB-T tuner

	
	Option 6
	4*ATSC tuner

	
	Option 7
	2*DVB-S/S2/S2X tuner + 2*DVB-C/T/ISDB-T tuner

	
	Option 8
	2*DVB-S/S2/S2X tuner + 2* ATSC tuner

	
	Option 9
	2*DVB-C/T/ISDB-T tuner + 2*ATSC tuner


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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