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FMUSER FUQ-4823C Multiplexer Scrambler 4 Tuner Inputs 5 MPTS Outputs DVB-S-DVB-S2-DVB-S2X UDP-RTP PID Remapping Web-Based NMS Satellite Broadcast IPTV
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Product overview
The FMUSER FUQ-4823C Multiplexer Scrambler processes DVB-S/S2/S2X signals through 4 tuner inputs and outputs 5 MPTS streams (4 bypassed + 1 multiplexed) via UDP/RTP. It remaps PIDs and multiplexes signals for efficient broadcast transmission. Features include web-based NMS and DiSEqC support for satellite control. Ideal for broadcast, satellite communication, and media distribution applications.
Key Features
- Supports multi-standard tuner inputs for DVB-S/S2/S2X signals across 950-2150MHz with ≤170 Mbps throughput.  
- Delivers flexible MPTS output with 4 bypassed and 1 multiplexed streams via UDP/RTP multicast/unicast.  
- Enables granular PID control with remapping of up to 256 PIDs per channel.  
- Features integrated management via web-based NMS and DiSEqC support.  
- Provides high-capacity processing for QPSK/8PSK/16APSK/32APSK constellations and FEC rates.  
Inner Principle Chart (Per Card)
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Specifications
	Input / Output
	4 Tuner input, F Type
5 MPTS (4 MPTS out thru bypassing, 1 MPTS multiplexing) out over UDP/RTP thru Data port, 100/1000Mself-adaption, unicast/multicast

	Mux
	Max number of managing PID: 256 (for 1 MPTS out thru multiplexing)

	
	Functions
	PID remapping (automatically/ manually)

	
	
	PID pass-through

	Tuner Section
	DVB-S
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	0.5~45 Msps

	
	
	Constellation
	QPSK

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	DVB-S2
	Input Frequency
	950-2150MHz

	
	
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps
32APSK:0.5~40 Msps

	
	
	Constellation
	QPSK/8PSK/16APSK/32APSK

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9,9/10
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10
32APSK: 3/4, 4/5, 5/6, 8/9

	
	
	Max input bitrate per tuner
	≤170 Mbps

	
	DVB-S2X
	Symbol Rate
	QPSK/8PSK/16APSK: 0.5~45 Msps;
8APSK/32APSK: 0.5~40 Msps

	
	
	Constellation
	QPSK/8PSK/16APSK/8APSK/32APSK

	
	
	FEC
	QPSK: 1/2, 3/5, 2/3, 3/4, 4/5, 5/6, 8/9, 9/10, 13/45, 9/20, 11/20
8PSK: 3/5, 2/3, 3/4, 5/6, 8/9, 9/10, 23/36, 25/36, 13/18
8APSK: 5/9-L, 26/45-L
16APSK: 2/3, 3/4, 4/5, 5/6, 8/9, 9/10,1/2-L, 8/15-L, 5/9-L, 26/45, 3/5, 3/5-L, 28/45, 23/36, 2/3-L, 25/36, 13/18, 7/9, 77/90
32APSK: 3/4, 4/5, 5/6, 8/9, 2/3-L, 32/45, 11/15, 7/9

	
	
	Max input bitrate per tuner
	≤170 Mbps

	
	Signal Strength
	-65 ~ -25dBm

	System
	Web management:100M NMS port

	
	Language: English and Chinese

	
	Ethernet software upgrade

	General
	Dimensions
	482mm×328mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz

	
	Consumption
	≤40W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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