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Product overview
The FUQ-8313 is a high-power DVB-T transmitter with selectable 800W/1000W/1200W RF output. It processes broadband signals in the 470–806MHz range using LDMOS amplification and AGC stabilization. The 2U rack-mount unit supports MFN/SFN topologies via modular design. Ideal for terrestrial TV broadcasting and emergency alert systems requiring low-distortion transmission.
Key feature
Provides front-panel LED/LCD for real-time fault monitoring 
Technical Specifications
 
	Input
	System standard
	DVB-(T)

	
	frequency
	470MHz~806MHz

	
	Input Level
	-20 dBm±3dB (87dbuv ±3dB)

	
	Input reflection loss
	≥15dB

	
	Input Interface
	‘N’

	Output
	RF output power
	800W/1000W/1200W optional

	
	Output frequency
	470MHz~806MHz
(For Single Channel: Every 8M available;
For Broadband Channel: consecutive 60M available)

	
	Output impedance
	50Ω

	
	frequency response
	±0.5dB

	
	Shoulder level
	≥36dB@central freqnencyIF±4.2MHz

	
	MER
	≥33dB

	
	output reflection loss
	≥20dB

	
	variation of output power
	±0.25dB

	
	In-band stray
	≤-60dBc

	
	Out-of-band suppression
	≥65dBc

	
	Output interface
	1-5/8

	General Parameters
	Working temperature
	-20~+50℃

	
	Storage temperature
	-30~+75℃

	
	Relatively humidity
	＜95% (25℃ no condensation)

	
	Cooling mode
	inside cooling fan

	
	atm press
	86~106kPa

	
	power supply
	AC, 220V±10%/50Hz

	
	Machine room requirement
	less dust, no shake

	
	Dimension(L×W×H)
	850mm×600mm×1695mm


 
System Diagram
 
[image: IMG_256]
PS: This diagram is a reference for 800W and 1000W transmitter.
For 1200W transmitter, there are 4 power amplifiers and 4 power supplier included.
 
Main Components List
	S/N
	Component Name
	Specs
	Qty
	Remarks

	1.  
	Final Power Amplifier
	300W
	3 pcs
	For 800W

	
	
	400W
	3 pcs
	For 1000W

	
	
	400W
	4 pcs
	For 1200W

	1.  
	Pre-Exciter
	 
	1 pc
	 

	1.  
	Monitor Unit
	 
	1 pc
	With LCD monitor on front door

	1.  
	Power Supply for
Final Amplifier
	 
	3 pcs
	For 800W/1000W

	
	
	 
	4 pcs
	For 1200W

	1.  
	Filter
	 
	1 pc
	As per order. (In case multiple single-channel transmitters are involved, a power combiner is required.)

	1.  
	Cabinet
	 
	1 pc
	 

	1.  
	Cooling Fan
	 
	1 set
	2 sets (with 1 set for backup) optional as order or needed

	Accessaries

	1.  
	Hard Feeder
	Φ40, 2 meter long
	1
	These parts are standard configuration. If there are special requirement, please indicate when place order.

	1.  
	Elbow
	 
	3
	

	1.  
	Hoop
	 
	3
	

	1.  
	Hose Clamp
	 
	13
	

	1.  
	Central Pin
	 
	3
	

	1.  
	Flange
	Φ40
	1
	

	1.  
	antenna
	 
	1
	As per order

	1.  
	Feeder
	 
	 
	As per order

	1.  
	Combiner
	 
	1
	As per order


 
Order Info
	Model Number
	Description

	DUT-8313(800W-I)
	800W Indoor

	DUT-8313(1000W-I)
	1000W Indoor

	DUT-8313(1200W-I)
	1200W Indoor


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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