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Product overview
The DUT-8323 is a high-power DVB-T transmitter delivering 1.5kW-3kW output through modular LDMOS amplifiers. It processes digital signals across 470-806MHz with AGC stability and supports both MFN and SFN network configurations. The 19" rack-mount unit features front-panel controls and LED monitoring for real-time diagnostics. Ideal for terrestrial TV broadcasting and large-scale digital transmission networks requiring scalable power output. 
Key feature
Multi-stage lightning protection and wide-voltage PSU (220V±10%) 
Technical Specifications
 
	Input
	System standard
	DVB-(T)

	
	frequency
	470MHz~806MHz

	
	Input Level
	-20 dBm±3dB (87dbuv ±3dB)

	
	Input reflection loss
	≥15dB

	
	Input Interface
	‘N’

	Output
	RF output power
	1500W/2000W/2500W/3000W optional

	
	Output frequency
	470MHz~806MHz
(For Single Channel: Every 8M available;
For Broadband Channel: consecutive 60M available)

	
	Output impedance
	50Ω

	
	frequency response
	±0.5dB

	
	Shoulder level
	≥36dB@central freqnencyIF±4.2MHz

	
	MER
	≥33dB

	
	output reflection loss
	≥20dB

	
	variation of output power
	±0.25dB

	
	In-band stray
	≤-60dBc

	
	Out-of-band suppression
	≥65dBc

	
	Output interface
	1-5/8

	General Parameters
	Working temperature
	-20~+50℃

	
	Storage temperature
	-30~+75℃

	
	Relatively humidity
	＜95% (25℃ no condensation)

	
	Cooling mode
	inside cooling fan

	
	atm press
	86~106kPa

	
	power supply
	AC, 220V±10%/50Hz

	
	Machine room requirement
	less dust, no shake

	
	Dimension(L×W×H)
	1050mm×600mm×1695mm


 
System Diagram
[image: IMG_256]
  
   PS: This diagram is a reference for 1500W and 2000W transmitter. For 2500W and 3000W transmitter,
          there are 4 power amplifiers and 8 power supplier included.
 
  Main Components List
	    S/N
	Component Name
	Specs
	Qty
	Remarks

	1.  
	Final Power Amplifier
	800W
	3 pcs
	For 2000W

	
	
	800W
	4 pcs
	For 3000W

	
	
	2000W and 3000W are standard power, 1500W and 2500W are customized version

	1.  
	Pre-Exciter
	 
	1 pc
	 

	1.  
	Monitor Unit
	 
	1 pc
	With LCD monitor on front door

	1.  
	Power Supply for
Final Amplifier
	 
	6 pcs
	For 1500W/2000W

	
	
	 
	8 pcs
	For 2500W/3000W

	1.  
	Filter
	 
	1 pc
	As per order. (In case multiple single-channel transmitters are involved, a power combiner is required.)

	1.  
	Cabinet
	 
	1 pc
	 

	1.  
	Cooling Fan
	 
	1 set
	2 sets (with 1 set for backup) optional as order or needed

	Accessaries

	1.  
	Hard Feeder
	Φ40, 2 meter long
	1
	These parts are standard configuration. If there are special requirement, please indicate when place order.

	1.  
	Elbow
	 
	3
	

	1.  
	Hoop
	 
	3
	

	1.  
	Hose Clamp
	 
	13
	

	1.  
	Central Pin
	 
	3
	

	1.  
	Flange
	Φ40
	1
	

	1.  
	antenna
	 
	1
	As per order

	1.  
	Feeder
	 
	 
	As per order

	1.  
	Combiner
	 
	1
	As per order


 
 
 
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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