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Product Overview 
The FMUSER FUQ-B System is an ATSC-compliant electronic program guide solution supporting 2044 transport streams and 69,905 programs. It generates PSI/SI standard tables with private descriptor support through Client/Service System mode. The 1U rack-mount unit features web-based control and supports 16-day EIT events. Ideal for digital TV headends, cable operators, and IPTV service providers requiring compliant EPG management.  
Key feature
 Web-based control interface for remote configuration 
 
Inner Principle
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Solution Guide
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Main Function
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Running Specs
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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Main Function
Program Association Table: STB searches programs with this table. PAT provides
PIDs for STB to get PMT and NIT.

Program Mapping Table: The Program Specific Information table that supplies basic
information about the services

PMT

Event Information Table: It contains info for events on defined virtual channels. STB
can display the program event in next few hours or days by reading this table.

System Time Table: It provides the current date and time of day info. The STB can
lay the system time by reading this table.

Master Guide Table: It lists version numbers, length in bytes, and PIDs for all of the
PSIP tables with exception of the STT which works independently from other tables.

Virtual Channel Table: It contail
Transport Stream.

st of attributes for virtual channels carrie

Rating Region Table: It carries rating info for multiple geographical regions.
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Hardware Requirement
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Software Requirement
—

EPG Server Configuration
cPU: 2.5GHz and above (recommended) Function Software:  EPG Software

Memory: 4GB and above Database: SQL Server 2005, SQL Server 2008
Hard disk: the free space is 20 GB and above

Network card:

1GB Network Card
100M Network Card (optional)

Operation System:

Windows server 2003, windows server 2008
(recommended)

EPG Client Configuration

CPU:
Memory:
Hard disk:
Network card:

2.0GHz and above (recommended)
2 GB and above
the free space is 2 GB and above

100M or 1GB Network Card

Function Software:

Operation System:

EPG Client Software

Windows XP (SP3 Above), Windows7
Windows Vista
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