[image: Fmuser标志1.png]Contact:Tomleequan    Email：sales@fmuser.com    whatsapp: +8613922702227
FMUSER FUQ-OSD100 OSD Logo Insertion Device 1-Channel Input DVB-ASI-IP Interfaces Broadcast-Grade Signal Processing Logo-OSD Overlay for TV Stations and Hotel IPTV
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Product overview
FMUSER OSD LOGO Insertion enables real-time logo/OSD overlay into broadcast streams via 1-channel DVB-ASI or IP input. The device preserves signal integrity during insertion, compliant with broadcast standards. Compact 1RU rack-mountable design with web-based control, ideal for television stations requiring on-screen branding and hospitality IPTV systems for customized guest content.
Key feature
Global client base with 20,000+ installations across 180+ countries
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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Dexin OSD Insertion Standard

’ Customization: Showing time &Displaying effect

’ Easy operation: fresh man learn it in few minutes

LOGO Insertion

Support jpg/jpeg/bmp/gif/png file

Support multi pictures compressed into a zip file and display pictures in a dynamic way

Multi transition type: Continuous/ Fade Inout/ Blind window/ Square
Custom live/wait time of pictures

Custom transparency D& /NG
Custom size DE OING—> vesin

Drag to move to any position

Transparent background
(hollow out) with png/gif
type picture

White background with
ipg/ipeg/bmp type picture

Caption Insertion — QR Code Insertion

Custom running direction & 9 Input URL and create immediately

EmgE
Custom running speed .Q_ D Support add text at top or bottom &
Custom font color/size/weight . A A ‘D Custom size: 40*40 -- 400*400
o]
Support multi languages - = €- 9 Support add logo at the center

Custom showing period and text length € @ Drag to move to any position

Custom background, transparency or any color €

Drag to move to any position
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