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Product overview:
The FUQ-XQR Transport Stream Player provides DVB-standard TS file playback through USB 2.0 input and DVB-ASI/BNC output. It processes 188-byte packet Transport Streams at 108Mbps for HD/SD signal generation. Built with P4-2.0G CPU and 256MB DDR memory, this 1U rack-mount unit supports MPEG-2/MPEG-4/H.264 standards. Ideal for broadcast equipment R&D validation, manufacturing line testing, and digital headend system demonstrations. 
Key feature: 
Engineering-grade stability: P4-2.0G CPU sustains 108Mbps continuous throughput 
Technical Specs:
 
	Interfaces
	INPUT: USB2.0

	
	OUTPUT: DVB ASI , BNC

	Packet Size
	188 bytes

	System Configurations
	OS: Windows 2000/XP Professional

	
	CPU: P4-2.0G

	
	Memory: 256M DDR

	
	Storage: 80G WD JB hard disk

	Applications
	Signal generator for developing DTV system and equipments

	
	Signal source for manufacturing of DTV system and equipments

	
	Demo of DTV system and equipment

	Physical/Environmental
	Dimension: 160×114×33 (mm )

	
	Weight: 0.5kg

	
	Operating temperature: 0℃～+55℃

	
	Operating humidity: 10%～80%


 

About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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