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The FMUSER FUQ-3514F modulator processes dual-channel DVB-ASI and SMPTE-310 inputs, delivering RF output from 50MHz to 860MHz. It employs ATSC 8-VSB modulation compliant with ATSC A/53 standard. Features adaptive digital pre-distortion (DPD) and remote control via IP and front panel. Ideal for ATSC broadcasting networks and set-top box testing applications. 
Key feature
Supports ATSC A/53 compliance for reliable digital broadcasting.  
Features dual-channel DVB-ASI/SMPTE-310 inputs with automatic switch-over.  
Delivers RF output from 50MHz to 860MHz with 1Hz stepping.  
Integrates adaptive digital pre-distortion (DPD) for signal optimization.  
Enables remote control via IP and front panel for monitoring and upgrades.
 
Specifications
 
	Input
	Self-adapted 2 Asi/SMPTE 310M input
2 ASI ports input, one for hot backup, BNC interface

	
	Dual IP input ports, one for hot backup , over UDP/RTP, Unicast/Multicast, GE ports

	
	1 channel 10MHz reference clock input

	Modulation
	Standard
	ATSC  A/53

	
	Constellation
	8VSB

	
	Bandwidth
	6 MHz

	
	FEC
	RS(208 188)+Trellis

	RF output
	Port
	N Type, 50Ω impedance

	
	RF range
	50~860Mhz,1Hz stepping

	
	Output Level ATT
	-20dBm~6dBm,0.1dB stepping

	
	Shoulder Level
	60dB

	
	MER
	≥ 40dB

	DPD
	Non-linear DPD
	over 10dB ACPR improvement (normally)

	
	linear DPD
	over 10dB non-flatness adjustment(normally)

	System
	LCD display & keyboard operation, NMS, Chinese & English operation display

	
	Software upgraded through network

	General
	Demission(WxLxH)
	482mm×455mm×44.5mm

	
	Weight
	6.0kg

	
	Temperature
	0~45℃( operation),-20~80℃( storage)

	
	Power Supply
	AC 110V±10%,50/60Hz or AC 220V±10%, 50/60Hz

	
	Consumption
	25W


 
 
Principle chart
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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