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The FUQ-3702 is an HD decoder supporting IP and ASI inputs with dual HD/SD-SDI outputs. It decodes signals to output high-quality video and audio. Features web-based management for remote control. Ideal for broadcast systems and professional video distribution.It is a 1-U case supporting both IP and ASI input. After decoding process, it outputs 2 channels of HD/SD-SDI videos with dual stereo audios embedded in each port. It also supports 1 IP (MPTS) output and featured with dual bi-directional ASI ports for input and output alternatively.
 
Key feature
Features dual IP inputs and single IP output handling MPTS/SPTS over UDP.,  
Includes bi-directional ASI ports for flexible input/output switching.,  
Outputs dual HD/SD-SDI channels with embedded stereo audio.,  
Supports MPEG-2, MPEG-4 AVC/H.264 video, and CC/Subtitle.,  
Enables web-based management via web server for easy operation. 
Principle Chart
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  Specification
 
	Input
	2 IP (MPTS/SPTS, 100M/1000Mbps Ethernet, RJ45, UDP protocol, Unicast/multicast)

	
	2* ASI bi-direction, BNC 75Ω

	Decode
	Video Format
	MPEG-2, MPEG4 AVC/H.264

	
	Interface
	2* SDI HD/SD

	
	Video Resolution
	480i, 480p, 576i, 576p, 720p@50/59.94/60, 1080i@50/59.94/60

	
	Audio Format
	MPEG1 Layer2, LC-AAC, HE-AAC, AC3 Passthrough

	
	Audio Channel
	dual stereo audios embedded in each port

	Output
	2*HD/SD-SDI decoding out

	
	0-2 ASI output

	
	1 IP output over UDP protocol

	General
	Operation
	Web-server

	
	Language
	Chinese/English

	
	Dimension (LxWxH)
	328 mm×482 mm×45mm

	
	Environment
	0~45℃(Work)；-20~80℃(Storage)

	
	Power Supply
	220VAC±10%，50Hz

	
	Consumption
	<25W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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