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Product Overview
The FMUSER FUQ-41019J decodes up to 8 IP or ASI inputs to CVBS outputs. It processes MPEG-2, H.264, AVS+ video and MPEG1 Layer 2, AC3 audio from transport streams. Featuring pluggable modules, LCD display, and web-server remote management, it is ideal for broadcast integration and reliable signal distribution.
 
Key feature
Supports 8 IP and 1 ASI inputs for versatile TS stream reception.
Delivers 8 channels of CVBS video and unbalanced stereo audio outputs.
Decodes MPEG-2, H.264, AVS+ video and MPEG1 Layer 2, AC3 audio.
Features real-time bit rate monitoring for optimized performance.
Managed via LCD display and web-server interface.
Principle Chart 
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Specification
	Input
	8*IP (MPTS/SPTS) (100Mbps Ethernet) (RJ45)

	
	IP Protocol
	UDP and RTP (Unicast/multicast)

	
	1* ASI (BNC)

	Decode
	Video Format
	MPEG-2/H.264/AVS+

	
	Interface
	8* CVBS（RCA）

	
	Video Resolution
	576i@25fps, 480i@29.97fps

	
	Audio Format
	MPEG-1 Layer 2, AC3 (2.0)

	
	Interface
	8*Unbalanced stereo (RCA)

	General
	Operation
	LCD display/Control button; Web-server

	
	Language
	Chinese/English

	
	Dimension (LxWxH)
	44 mm×482 mm×410mm

	
	Environment
	0~45℃(Work)；-20~80℃(Storage)

	
	Power Supply
	220VAC±10%，50Hz

	
	Consumption
	<25W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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