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The FUQ-4216B ISDB-T Multiplexer is a dual-channel TS re-multiplexer with 12 ASI inputs and 2 IP outputs over UDP. It processes transport streams by re-multiplexing, editing PSI/SI tables, and generating IIP packets. Supporting remote upgrades and network management, this device is ideal for broadcast headend applications in regions like Japan and South America. 
Key feature
Supports dual-channel TS re-multiplexing compliant with ISDB-T/ISDB-Tb standards.  
Enables PSI/SI table editing and IIP packet generation.  
Features 12 ASI inputs and 2 IP outputs over UDP.  
Facilitates SFN operations and hierarchical transmission.  
Includes PID filtering/re-mapping and accurate PCR adjusting.
Specifications
	Signal inputting
	12 ASI input

	
	188/204Byte transmission stream packet

	
	TS packet mode and suddenly code rate mode

	
	GPS 10mhz reference clock inputting

	
	GPS 1pps signal inputting

	Re-multiplexing
	2 separate channels TS re-multiplexer

	
	PCR accurate adjusting

	
	PSI/SI table automatically generating

	Modulation parameter
	mode：mode1(2k)    mode2(4k)    mode3(8k)

	
	Guard interval：1/4   1/8  1/16   1/32

	
	Coding rate：1/2   2/3  3/4   5/6   7/8

	
	constellation：DQPSK  QPSK  16QAM  64QAM

	
	Layer：A      A+B    A+B+C

	
	Bandwidth: 6MHz    7MHz     8MHz

	SFN parameter
	Maximum time delay：0ms ～ 1000ms

	
	Off set：-1000ms ～ +1000ms

	
	Device ID ：01 ～ 30

	Output
	2 ASI output(BNC)

	
	2 IP output(UDP protocol)

	
	  RS encoding output supporting

	
	GPS 1pps and GPS 10Mhz loop-out(BNC)

	General
	Demission：44mmx482mmx410mm

	
	Temperature：0～45℃(operation)    -20～80℃（storage）

	
	Power supply：220VAC±10%，50/60Hz，10W


 
Principle Chart
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About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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