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FMUSER FUQ-4312D 4-input SD Encoder CVBS-S-Video-SD-SDI MPEG-2 AES-EBU Audio TS over UDP output Broadcast Headend System
[bookmark: _GoBack][image: 3EEECN_20180122011505]Product overview
The FMUSER FUQ-4312D is a professional MPEG-2 SD encoder with 4 inputs (CVBS, S-Video, SD-SDI, and analog/AES/EBU audio). It processes PAL/NTSC signals (720×480/576) with de-interlacing and outputs ASI or UDP/IP transport streams. This 1U rack-mount unit supports dual control via LCD and web interface, ideal for broadcast headends and IP-based contribution networks.
Key feature
Controls via LCD panel & web interface with GOP customization 
Principle Chart
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Specifications
 
	input
	Video
	Analog composite video(CVBS), BNC interface

	
	
	S-Video interface

	
	
	SD-SDI, BNC interface

	
	Audio
	Analog stereo audio(balanced), XLR interface

	
	
	Analog stereo audio(unbalanced), BNC interface

	
	
	AES / EBU digital audio, XLR interface

	
	
	SD-SDI embedded audio

	Video
	Resolution
	720×480_59.94i, 720×576_50i

	
	Encoding
	MPEG-2 MP@ML

	
	Bit-rate
	0.8Mbps~19.5Mbps

	
	Rate Control
	CBR/VBR

	
	GOP Structure
	IIII, IPPP, IBPB, IBBP

	
	Aspect Ratio
	4:3; 16:9

	
	Advanced Pretreatment
	De-interlacing, noise reduction, sharpening

	Audio
	Encoding
	MPEG-1 Layer 2

	
	Sampling rate
	48KHz, 44.1KHz, 32KHz

	
	Bitrate
	64Kbps—384Kbps

	Stream output
	2-way ASI output, BNC interface

	
	E1 output –Optional

	
	TS output over UDP,100/1000Base-T Ethernet interface (UDP unicast / multicast)

	System function
	LCD/keyboard, network management(NMS)
Chinese and English language

	
	Ethernet software upgrade

	General
	Dimensions
(WxDxH)
	482mm×455mm×44.5mm

	
	Temperature range
	0~45℃(operation), -20~80℃(storage)

	
	Power Requirements
	AC 110V±10%,50/60Hz or AC 220V±10%,50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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