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FMUSER FUQ-4315B 4-Channel Encoder 4× CVBS-S-Video-YPbPr Input ASI-IP Output MPEG-2 MPEG-1 Layer II Encoding Multiplexing for Cable Headends Satellite Broadcasting
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The FUQ-4315E is a 4-channel encoder with CVBS/S-Video/YPbPr inputs, supporting MPEG-2 video and MPEG-1 Layer II audio encoding. It processes signals through ASI input multiplexing to generate MPTS streams, with outputs via IP and ASI. This unit features LCD+keyboard control and Web NMS/SNMP management. Ideal for digital headends in cable and satellite broadcasting systems. 
Key feature 
- Integrates 4× CVBS/S-Video/YPbPr inputs and 1× ASI input for flexible signal integration.  
- Supports MPEG-2 video encoding at 1-19.5Mbps and MPEG-1 Layer II audio encoding.  
- Provides ASI and IP outputs with UDP/RTP multicast/unicast capability.  
- Ensures stream stability through CBR and PCR adjustment.  
- Enables PSI/SI editing and PID remapping/passthrough, managed via LCD+keyboard or Web NMS/SNMP.  
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Specifications
	Input
	4xS-Video/YPbPr/CVBS (RCA)

	
	1×ASI input

	Encoding
	Video
	Format
	MPEG-2 MP@ML (4:2:0)

	
	
	Interface
	S-Video/YPbPr/CVBS*4(RCA)

	
	
	Bitrate
	1-19.5Mbps

	
	
	Resolution
	720*480_60i, 720*576_50i

	
	
	Rate mode
	VBR/CBR

	
	
	Chroma
	4:2:0

	
	
	Aspect
	16:9,4:3, 1:1, 2.21:1

	
	Audio
	Format
	MPEG1 Layer II

	
	
	Interface
	4*Stereo or 8*mono (RCA)

	
	
	Sample rate
	48KHz

	
	
	Bitrate
	64kbps,96kbps,128kbps,192kbps,256kbps,320kbps

	Stream output
	1*ASI

	
	1 IP over UDP/RTP, 10/100Base-T Ethernet interface (unicast / multicast)

	System
	Local interface
	LCD + control buttons

	
	Remote management
	Web NMS Management

	
	Language
	English

	General
	Dimension
(W*D*H)
	482mm×300mm×44.5mm

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power
	AC 100V~240V

	
	Consumption
	25W


           
 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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