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Product Overview
The FMUSER FUQ-4344 is a professional audio encoder with dual unbalanced stereo inputs for backup redundancy. It encodes audio using MPEG-1 Layer II compression and adjustable gain. Control is via web-based NMS and LCD/keyboard. Ideal for broadcast systems requiring reliable transmission through ASI and IP over UDP outputs. 
Key feature
Supports dual unbalanced stereo inputs with backup for enhanced reliability.  
Encodes audio using MPEG-1 Layer II with bit-rates from 32 to 384 Kb/s.  
Features adjustable audio gain control from -20 to +6 dB.  
Provides ASI and IP over UDP outputs for versatile transmission.  
Enables management via web-based NMS and LCD/keyboard operation.  
Principle Chart
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Specifications
	Audio Encode
	Interface
	2 pairs of unbalanced stereo inputs(one for backup), BNC interface

	
	Encoding Format
	MPEG1 Layer 2

	
	Audio Gain
	-20 ~ +6 dB

	
	Sampling Rate
	48KHz

	
	Bit-rate
	32/48/56/64/80/96/112/128/160/192/224/256/320/384Kb/s

	Stream output
	1*ASI output, BNC interface

	
	IP output over UDP mirror ASI output, 100M Base-T Ethernet interface (unicast/multicast)

	System
	LCD/keyboard operating, web-based NMS manage

	
	Language: LCD English
Web Chinese

	
	Ethernet software & hardware upgrade

	Miscellaneous
	Dimension
	164mm×128mm×45mm (W× L× H)

	
	Approx weight 
	＜1kg

	
	Temperature
	0~45℃ (work),  -20~80℃（Storage）

	
	Power supply
	DC12V


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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