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The FMUSER FUQ-4415B is a DVB-T modulator with 128 IP inputs over UDP/RTP and outputs 4 DVB-T carriers and 4 MPTS streams. It integrates multiplexing and modulating functions for efficient signal processing. Features web-based NMS management for easy control. Ideal for DTV broadcasting systems, providing reliable transmission in modern headend setups.
Key feature
Enables web-based NMS management for monitoring and configuration. 
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Specifications
	Input
	128 IP(SPTS/MPTS) input over UDP and RTP, RJ45, 1000M/100M, Unicast/Multicast         

	Multiplexing
	Maximum PID Remapping
	256 per input channel

	
	Function
	PID Remapping

	
	
	Accurate PCR adjusting

	
	
	Generate PSI/SI table automatically

	Modulation
	DVB-T
	Standard
	EN300744

	
	
	FFT mode
	2K

	
	
	Bandwidth
	6M, 7M, 8M

	
	
	Constellation
	QPSK, 16QAM, 64QAM

	
	
	Guard Interval
	1/4, 1/8, 1/16, 1/32

	
	
	FEC
	1/2, 2/3, 3/4, 5/6, 7/8

	
	
	MER
	≥42 dB

	
	
	RF frequency
	50~960MHz, 1KHz step

	
	
	RF out
	1 RF port

	
	
	
	4*DVB-T non-adjacent carriers combined output , 40M total bandwidth limitation

	
	
	RF output level
	-28~ -3 dBm, 0.1db step

	Stream Out
	4*MPTS over UDP and RTP out (RJ45, 1000M/100M Unicast/Multicast)

	System
	LCD/Keyboard operating and web-based NMS support

	
	Ethernet software upgrading

	General
	Dimension
(W*D*H)
	482mm×300mm×44.5mm

	
	Temperature
	0~45℃(Operation) ; -20~80℃(Storage)

	
	Power supply
	AC 100V±1050/60Hz; AC 220V±10%, 50/60HZ


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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