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The FUQ-4619B ASI to IP Gateway converts 8 ASI inputs to IP outputs, supporting SPTS streams with BISS descrambling over UDP/RTP protocols. It processes signals by descrambling and filtering for efficient IP conversion. Controlled via SNMP for network management, this device suits broadcast head-end systems and IPTV distribution networks. 
Key feature
Supports 8-channel ASI input for conversion to SPTS streams.  
Provides BISS descrambling (Mode 1/E) with 120Mbps throughput.  
Features 1 GE output with configurable bit-rates: 400Mbps or 800Mbps.  
Includes IP null packet filtering and multi-protocol support (UDP, RTP/RTSP, unicast/multicast).
Principle Chart
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Specification
 
	Input
	8 ASI input                                             

	Output
	1 GE output, UDP, RTP/RTSP protocol, unicast and Multicast
256 SPTS output — Without BISS function and IP null packet filter
32 SPTS output — Without BISS function
20 SPTS output — With BISS function

	BISS descrambling
	Mode 1, Mode E

	Transmission Bit-rate
	Maximum total bit-rate is 400Mbps—256 SPTS output

	
	Maximum total bit-rate is 800Mbps—32/20 SPTS output

	General
	Dimension(WxLxH)
	482mm×410mm×44mm

	
	Weight
	3.6kg

	
	Temperature
	0~45℃(working )，-20~80℃(storage)

	
	Power supply
	100~240VAC，50/60Hz

	
	consumption
	20W


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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