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Product overview
The FMUSER FUQ-4713 is a DVB-ASI distribution hub with 2 inputs and 24 outputs (6×4 groups) for digital TV signal routing. It processes 1-216Mbps ASI signals with synchronized output replication. Features LCD display, front-panel keyboard, and SNMP-based NMS for remote monitoring. Ideal for broadcast headends and CATV systems requiring multi-device signal distribution. 
Key feature
Operates at 220VAC±10%, 50Hz with 0-45°C operating temperature range
 
Specifications
	Interface
	Input interface
	DVB ASI

	
	Input interface number
	2

	
	Output interface
	DVB ASI

	
	Output interface number
	24

	Interface Specification
	ASI
	DVB Standard

	Code rate
	1-216Mbps

	Miscellaneous
	Dimension
	44mm x 482mm x 410mm

	
	Temperature
	0-45℃(Operation); -20 – 80℃ (Storage)

	
	Power
	220VAC± 10%, 50Hz, 10W


 

About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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