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The FMUSER FUQ-100B is a multiplexer and scrambler supporting 8 ASI and 64 IP inputs. It processes signals with PID re-mapping and EPG insertion, outputting TS streams via ASI and IP ports. With web-based NMS management, it suits digital TV head-end systems and CATV broadcasting. 
Key feature
Supports 8 ASI inputs and 64 IP inputs via UDP protocol.
Features multiplexing, scrambling, PID re-mapping, and PSI/SI editing.
Compliant with ISO13818, EN300 468, and simulcrypt standards.
Includes 2 groups of ASI outputs (each with 2 channels) and IP outputs.
Offers web-based NMS management for easy control.
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Specifications
	Input
	8 ASI input+64 IP input DATA 1 and DATA 2 over UDP protocol

	Re-multiplex
	PID re-mapping

	
	PCR accurate adjusting

	
	PSI/SI (PAT, PMT) tables auto generation and edition

	Scrambling
	Simul-crypt CA
	6

	
	Standard
	ETR289, ETSI 101 197, ETSI 103 197

	
	Connection
	Local/Remote connect

	Output port
	ASI
	2 groups separate outputs (each group has 2 channels)

	
	IP
	MPTS over UDP, RTP/RTSP output (RJ45), 1000Mbps Ethernet, DATA 1 and DATA 2

	PID
	Output range
	0x0000—0x1FFF

	
	PID transparent
	Any PID transparent and mapping achievable

	
	Amount of output PID
	512

	NMS port
	Ethernet port
	10/100M/1000M self adaption

	General
	Dimensions
	482mm×300mm×44mm (WxLxH)

	
	Weight
	3.5kg

	
	Temperature
	0~45℃(operation), -20~80℃(storage)

	
	Power supply
	AC 110V±10%, 50/60Hz Or AC 220V±10%, 50/60Hz


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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NDS3712B Multiplexer Scrambler
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