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FMUSER FUQ-5315K Encoder 4-8-12 HDMI Inputs IP Output MPEG-4 AVC-H264 LC-AAC-HE-AAC Web Management for IP Broadcasting
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Product Overview
The FMUSER FUQ-5315K is a multi-channel encoder with 4/8/12 HDMI inputs, supporting MPEG-4 AVC/H.264 video and LC-AAC/HE-AAC audio encoding. It streams content via UDP, RTSP, RTMP, HTTP, and HLS protocols for reception on PCs and mobile devices. Controlled through web-based management, it enables easy updates. Ideal for professional IP broadcasting in live streaming and digital media distribution. 
Key feature
Allows control and updates via web-based management.* Support MPEG-4 AVC/H.264 video encoding and LC-AAC or HE-AAC Audio encoding
Inner Principle Chart (Per Module)
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Specifications
	Input
	4/8/12 HDMI inputs

	Encoder
Section
	Video
	Resolution
 
	Input
	Output

	
	
	
	1920x1080_60p, 1920x1080_60i
	1920x1080_30p

	
	
	
	1920x1080_50p, 1920x1080_50i
	1920x1080_25p

	
	
	
	1280x720_60p
	1280x720_30p

	
	
	
	1280x720_50p
	1280x720_25p

	
	
	
	720x480_60i
	720x480_30p

	
	
	
	720x576_50i
	720x576_25p

	
	
	Encoding
	MPEG-4 AVC/H.264 (Baseline profile, Main profile, High profile)

	
	
	Bit rate
	1Mbps~13Mbps

	
	
	Rate Mode
	CBR, VBR

	
	
	GOP Size
	25~50

	
	Audio
	Encoding
	LC-AAC or HE-AAC

	
	
	Sampling rate
	48KHz input, 44.1KHz output

	
	
	Bitrate
	LC-AAC : 48, 64, 96, 128, 256 kbps
HE-AAC : 48, 64 kbps

	Stream out
	IP out over UDP (Unicast/Multicast) , RTSP, RTMP, HTTP, HLS (RJ45, 100M )
ASI output port and Data port are not applicable currently

	System
	Remote control
	Network management (WEB)

	
	Language
	Chinese and English

	
	Upgrade
	Ethernet software upgrade

	General
	Operation temperature
	0~45℃(work), -20~80℃（Storage）

	
	Power supply
	AC 100-240V 50/60Hz 2A

	
	Dimensions
	482mm×328mm×44mm


 


About Us
  FMUSER is a company specializing in broadcasting and television transmission systems and integrating hotel IPTV systems. The company was established in 2009 and has served over 180 countries worldwide. More than 20,000 television stations, radio stations, and hotel clients from different.
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